<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle>
    <drawing>
        <library name="Upverter Library">
            <description>Upverter Parts Library

Created by Upverter.com</description>
            <packages>
                <package name="MICROCHIP_PIC18F2550-I-SO_0">
                    <description></description>
                </package>
            </packages>
            <symbols>
                <symbol name="MICROCHIP_PIC18F2550-I-SO_0_0">
                    <description></description>
                    <pin name="!MCLR/VPP/RE3"/>
                    <pin name="RA0/AN0"/>
                    <pin name="RA1/AN1"/>
                    <pin name="RA2/AN2/VREF-/CVREF"/>
                    <pin name="RA3/AN3/VREF+"/>
                    <pin name="RA4/T0CKI/C1OUT/RCV"/>
                    <pin name="RA5/AN4/!SS/HLVDIN/C2OUT"/>
                    <pin name="VSS"/>
                    <pin name="OSC1/CLKI"/>
                    <pin name="OSC2/CLKO/RA6"/>
                    <pin name="RC0/T1OSO/T13CKI"/>
                    <pin name="RC1/T1OSI/CCP2/!UOE"/>
                    <pin name="RC2/CCP1"/>
                    <pin name="VUSB"/>
                    <pin name="RC4/D-/VM"/>
                    <pin name="RC5/D+/VP"/>
                    <pin name="RC6/TX/CK"/>
                    <pin name="RC7/RX/DT/SDO"/>
                    <pin name="VSS2"/>
                    <pin name="VDD"/>
                    <pin name="RB0/AN12/INT0/FLT0/SDI/SDA"/>
                    <pin name="RB1/AN10/INT1/SCK/SCL"/>
                    <pin name="RB2/AN8/INT2/VMO"/>
                    <pin name="RB3/AN9/CCP2/VPO"/>
                    <pin name="RB4/AN11/KBI0"/>
                    <pin name="RB5/KBI1/PGM"/>
                    <pin name="RB6/KBI2/PGC"/>
                    <pin name="RB7/KBI3/PGD"/>
                </symbol>
            </symbols>
            <devicesets>
                <deviceset prefix="U" name="MICROCHIP_PIC18F2550-I-SO">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="MICROCHIP_PIC18F2550-I-SO_0_0"/>
                    </gates>
                    <devices>
                        <device name="MICROCHIP_PIC18F2550-I-SO_0_0" package="MICROCHIP_PIC18F2550-I-SO_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="!MCLR/VPP/RE3"/>
                                <connect gate="G$0" pad="2" pin="RA0/AN0"/>
                                <connect gate="G$0" pad="3" pin="RA1/AN1"/>
                                <connect gate="G$0" pad="4" pin="RA2/AN2/VREF-/CVREF"/>
                                <connect gate="G$0" pad="5" pin="RA3/AN3/VREF+"/>
                                <connect gate="G$0" pad="6" pin="RA4/T0CKI/C1OUT/RCV"/>
                                <connect gate="G$0" pad="7" pin="RA5/AN4/!SS/HLVDIN/C2OUT"/>
                                <connect gate="G$0" pad="8" pin="VSS"/>
                                <connect gate="G$0" pad="9" pin="OSC1/CLKI"/>
                                <connect gate="G$0" pad="10" pin="OSC2/CLKO/RA6"/>
                                <connect gate="G$0" pad="11" pin="RC0/T1OSO/T13CKI"/>
                                <connect gate="G$0" pad="12" pin="RC1/T1OSI/CCP2/!UOE"/>
                                <connect gate="G$0" pad="13" pin="RC2/CCP1"/>
                                <connect gate="G$0" pad="14" pin="VUSB"/>
                                <connect gate="G$0" pad="15" pin="RC4/D-/VM"/>
                                <connect gate="G$0" pad="16" pin="RC5/D+/VP"/>
                                <connect gate="G$0" pad="17" pin="RC6/TX/CK"/>
                                <connect gate="G$0" pad="18" pin="RC7/RX/DT/SDO"/>
                                <connect gate="G$0" pad="19" pin="VSS2"/>
                                <connect gate="G$0" pad="20" pin="VDD"/>
                                <connect gate="G$0" pad="21" pin="RB0/AN12/INT0/FLT0/SDI/SDA"/>
                                <connect gate="G$0" pad="22" pin="RB1/AN10/INT1/SCK/SCL"/>
                                <connect gate="G$0" pad="23" pin="RB2/AN8/INT2/VMO"/>
                                <connect gate="G$0" pad="24" pin="RB3/AN9/CCP2/VPO"/>
                                <connect gate="G$0" pad="25" pin="RB4/AN11/KBI0"/>
                                <connect gate="G$0" pad="26" pin="RB5/KBI1/PGM"/>
                                <connect gate="G$0" pad="27" pin="RB6/KBI2/PGC"/>
                                <connect gate="G$0" pad="28" pin="RB7/KBI3/PGD"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="579-PIC18F2550-I/SO"/>
                                    <attribute name="Flash" value="32KB"/>
                                    <attribute name="ipc_land_pattern_name" value="SOIC127P1030X250-28"/>
                                    <attribute name="temperature_range_high" value="+85°C"/>
                                    <attribute name="MPN" value="PIC18F2550-I/SO"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="digikey_description" value="IC MCU 8BIT 32KB FLASH 28SOIC"/>
                                    <attribute name="digikey_part_number" value="PIC18F2550-I/SO-ND"/>
                                    <attribute name="RAM" value="2KB"/>
                                    <attribute name="prefix" value="U"/>
                                    <attribute name="datasheet" value="https://upverter.com/datasheet/8e44134229eeba9b89b2ef331b5253295cf39cdc.pdf"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="mfg_package_ident" value="C04-052C"/>
                                    <attribute name="voltage" value=""/>
                                    <attribute name="temperature_range_low" value="-40°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="Core_Size" value="8-Bit"/>
                                    <attribute name="MF" value="Microchip"/>
                                    <attribute name="package" value="SOIC28"/>
                                    <attribute name="Speed" value="48MHz"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
            </devicesets>
        </library>
    </drawing>
</eagle>
