<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle>
    <drawing>
        <library name="Upverter Library">
            <description>Upverter Parts Library

Created by Upverter.com</description>
            <packages>
                <package name="ON_SEMI_MMBT4401LT3G_0">
                    <description></description>
                </package>
                <package name="HIROSE_DF11CZ-16DS-2V_22_0">
                    <description></description>
                </package>
                <package name="MICROCHIP_93LC56B-I-SN_0">
                    <description></description>
                </package>
                <package name="JST_BM12B-SRSS-TB_LF_SN_0">
                    <description></description>
                </package>
                <package name="SAMSUNG_SIP-007AFS001_0">
                    <description></description>
                </package>
                <package name="VISHAY_CRCW0805200RFKEA_0">
                    <description></description>
                </package>
                <package name="BOURNS_SRN6045-6R8Y_0">
                    <description></description>
                </package>
                <package name="CTS_218-6LPST_0">
                    <description></description>
                </package>
                <package name="TEXAS_INSTRUMENTS_SN74AVC2T244DQMR_0">
                    <description></description>
                </package>
                <package name="EPSON_FA-20H_16.0000MF12V-AJ3_0">
                    <description>MHz Range Crystal Unit</description>
                </package>
                <package name="SILICON_LABORATORIES_CP2102-GMR_0">
                    <description></description>
                </package>
                <package name="IXYS_CPC1927J_0">
                    <description></description>
                </package>
                <package name="TEXAS_INSTRUMENTS_BQ294700DSGR_0">
                    <description></description>
                </package>
                <package name="TEXAS_INSTRUMENTS_BQ24259RGER_0">
                    <description></description>
                </package>
                <package name="BOURNS_PEC16-4220F-S0024_0">
                    <description></description>
                </package>
                <package name="AVX_F950J476MPAAQ2_0">
                    <description></description>
                </package>
                <package name="PANASONIC_ERJ-3EKF22R0V_0">
                    <description></description>
                </package>
                <package name="ST_MICROELECTRONICS_L7805CDT-TR_0">
                    <description></description>
                </package>
                <package name="TEXAS_INSTRUMENTS_TLC5955RTQR_0">
                    <description></description>
                </package>
                <package name="DIODES_MMSZ5233B_0">
                    <description></description>
                </package>
                <package name="E-SWITCH_TL1015AF160QG_0">
                    <description></description>
                </package>
                <package name="TEXAS_INSTRUMENTS_AM4376BZDN100_0">
                    <description></description>
                </package>
                <package name="ANALOG_DEVICES_INC._ADV7180BSTZ_0">
                    <description></description>
                </package>
                <package name="TEXAS_INSTRUMENTS_TPS65218B1RSLT_0">
                    <description></description>
                </package>
                <package name="TEXAS_INSTRUMENTS_TPS62160DSGR_0">
                    <description></description>
                </package>
                <package name="JST_SM02B-SRSS-TB_LF_SN_0">
                    <description></description>
                </package>
                <package name="TEXAS_INSTRUMENTS_LMP7702MA_0">
                    <description></description>
                </package>
                <package name="VISHAY_SIA519EDJ-T1-GE3_0">
                    <description>Mosfet Array N and P-Channel 20V 4.5A 7.8W Surface Mount PowerPAK® SC-70-6 Dual</description>
                </package>
                <package name="MICRON_TECHNOLOGY_INC._MT29F256G08CMCABH2-12Z_0">
                    <description></description>
                </package>
            </packages>
            <symbols>
                <symbol name="ON_SEMI_MMBT4401LT3G_0_0">
                    <description></description>
                    <pin name="BASE"/>
                    <pin name="COLLECTOR"/>
                    <pin name="EMITTER"/>
                </symbol>
                <symbol name="HIROSE_DF11CZ-16DS-2V_22_0_0">
                    <description></description>
                    <pin name="1"/>
                    <pin name="2"/>
                    <pin name="3"/>
                    <pin name="4"/>
                    <pin name="5"/>
                    <pin name="6"/>
                    <pin name="7"/>
                    <pin name="8"/>
                    <pin name="9"/>
                    <pin name="10"/>
                    <pin name="11"/>
                    <pin name="12"/>
                    <pin name="13"/>
                    <pin name="14"/>
                    <pin name="15"/>
                    <pin name="16"/>
                    <pin name="MNT_1"/>
                    <pin name="MNT_2"/>
                </symbol>
                <symbol name="MICROCHIP_93LC56B-I-SN_0_0">
                    <description></description>
                    <pin direction="pwr" name="VCC"/>
                    <pin direction="in" name="CLK"/>
                    <pin direction="in" name="CS"/>
                    <pin direction="in" name="DI"/>
                    <pin direction="out" name="DO"/>
                    <pin name="NC"/>
                    <pin name="NC2"/>
                    <pin direction="pwr" name="VSS"/>
                </symbol>
                <symbol name="JST_BM12B-SRSS-TB_LF_SN_0_0">
                    <description></description>
                    <pin name="1"/>
                    <pin name="2"/>
                    <pin name="3"/>
                    <pin name="4"/>
                    <pin name="5"/>
                    <pin name="6"/>
                    <pin name="7"/>
                    <pin name="8"/>
                    <pin name="9"/>
                    <pin name="10"/>
                    <pin name="11"/>
                    <pin name="12"/>
                    <pin name="MNT_1"/>
                    <pin name="MNT_2"/>
                </symbol>
                <symbol name="SAMSUNG_SIP-007AFS001_0_0">
                    <description></description>
                    <pin name="AP_GPA13"/>
                    <pin name="AP_GPA14"/>
                    <pin name="AP_GPA9"/>
                    <pin name="AP_GPA15"/>
                    <pin name="AP_GPA12"/>
                    <pin name="AP_GPA4"/>
                    <pin name="AP_GPA5"/>
                    <pin name="AP_GPA16"/>
                    <pin name="AP_GPA11"/>
                    <pin name="AP_GPB11"/>
                    <pin name="AP_GPB18"/>
                    <pin name="AP_GPC25"/>
                    <pin name="AP_GPE31"/>
                    <pin name="AP_GPC17"/>
                    <pin name="AP_GPC0"/>
                    <pin name="AP_GPC26"/>
                    <pin name="AP_GPB8"/>
                    <pin name="AP_GPA20"/>
                    <pin name="AP_GPA18"/>
                    <pin name="AP_GPA21"/>
                    <pin name="AP_GPA10"/>
                    <pin name="AP_GPA6"/>
                    <pin name="AP_GPD8"/>
                    <pin name="AP_GPE30"/>
                    <pin name="AP_GPC27"/>
                    <pin name="AP_GPB22"/>
                    <pin name="AP_GPB23"/>
                    <pin name="AP_GPA22"/>
                    <pin name="AP_GPA19"/>
                    <pin name="AP_GPA17"/>
                    <pin name="AP_GPA3"/>
                    <pin name="GMAC_TXEN"/>
                    <pin name="GMAC_TXD1"/>
                    <pin name="GMAC_TXD3"/>
                    <pin name="GMAC_GTXCLK"/>
                    <pin name="GMAC_RXDV"/>
                    <pin name="GMAC_RXD2"/>
                    <pin name="GMAC_RXD0"/>
                    <pin name="GMAC_TXD0"/>
                    <pin name="GMAC_TXD2"/>
                    <pin name="GMAC_MDC"/>
                    <pin name="GMAC_RXCLK"/>
                    <pin name="GMAC_RXD3"/>
                    <pin name="GMAC_RXD1"/>
                    <pin name="GMAC_MDIO"/>
                </symbol>
                <symbol name="SAMSUNG_SIP-007AFS001_0_1">
                    <description></description>
                    <pin name="VCC5P0_OTGVBUS"/>
                    <pin name="VCC5P0_OTGVBUS2"/>
                    <pin name="VCC2P8_LDO7"/>
                    <pin name="VCC2P8_LDO72"/>
                    <pin name="VCC2P8_LDO73"/>
                    <pin name="VCC_LDO5"/>
                    <pin name="VCC_LDO52"/>
                    <pin name="VCC_LDO53"/>
                    <pin name="VCC_LDO2"/>
                    <pin name="VCC_LDO22"/>
                    <pin name="VCC_LDO23"/>
                    <pin name="VCC_LDO1"/>
                    <pin name="VCC_LDO12"/>
                    <pin name="VCC_LDO13"/>
                    <pin name="VCC1P2_LDO10"/>
                    <pin name="VCC1P2_LDO102"/>
                    <pin name="VCC1P2_LDO103"/>
                    <pin name="VCC1P8_LDO4"/>
                    <pin name="VCC_LDO9"/>
                    <pin name="VCC1P8_LDO42"/>
                    <pin name="VCC_LDO92"/>
                    <pin name="VCC_LDO93"/>
                    <pin name="VCC1P8_LDO43"/>
                    <pin name="VBAT_MAIN"/>
                    <pin name="VBAT_MAIN2"/>
                    <pin name="VBAT_MAIN3"/>
                    <pin name="VBAT_MAIN4"/>
                    <pin name="VBAT_MAIN5"/>
                    <pin name="VBAT_MAIN6"/>
                    <pin name="VBAT_MAIN7"/>
                    <pin name="VBAT_MAIN8"/>
                    <pin name="VBAT_MAIN9"/>
                    <pin name="VBAT_MAIN10"/>
                    <pin name="VCC3V3_LDO8"/>
                    <pin name="VCC3V3_LDO82"/>
                    <pin name="VCC3V3_LDO83"/>
                    <pin name="VCC3P3_SYS"/>
                    <pin name="VCC3P3_SYS2"/>
                    <pin name="VCC3P3_SYS3"/>
                    <pin name="VCC3P3_SYS4"/>
                    <pin name="TP"/>
                    <pin name="TP2"/>
                    <pin name="TP3"/>
                    <pin name="TP4"/>
                    <pin name="TP5"/>
                    <pin name="TP6"/>
                    <pin name="TP7"/>
                    <pin name="TP8"/>
                    <pin name="TP9"/>
                    <pin name="TP10"/>
                    <pin name="TP11"/>
                    <pin name="TP12"/>
                    <pin name="TP13"/>
                    <pin name="TP14"/>
                    <pin name="TP15"/>
                    <pin name="TP16"/>
                    <pin name="TP17"/>
                    <pin name="TP18"/>
                    <pin name="TP19"/>
                    <pin name="TP20"/>
                    <pin name="GND"/>
                    <pin name="GND2"/>
                    <pin name="GND3"/>
                    <pin name="GND4"/>
                    <pin name="GND5"/>
                    <pin name="GND6"/>
                    <pin name="GND7"/>
                    <pin name="GND8"/>
                    <pin name="GND9"/>
                    <pin name="GND10"/>
                    <pin name="GND11"/>
                    <pin name="GND12"/>
                    <pin name="GND13"/>
                    <pin name="GND14"/>
                    <pin name="GND15"/>
                    <pin name="GND16"/>
                    <pin name="GND17"/>
                    <pin name="GND18"/>
                    <pin name="GND19"/>
                    <pin name="GND20"/>
                    <pin name="GND21"/>
                    <pin name="GND22"/>
                    <pin name="GND23"/>
                    <pin name="GND24"/>
                    <pin name="GND25"/>
                    <pin name="GND26"/>
                    <pin name="GND27"/>
                    <pin name="GND28"/>
                    <pin name="GND29"/>
                    <pin name="GND30"/>
                    <pin name="GND31"/>
                    <pin name="GND32"/>
                    <pin name="GND33"/>
                    <pin name="GND34"/>
                    <pin name="GND35"/>
                    <pin name="GND36"/>
                    <pin name="GND37"/>
                    <pin name="GND38"/>
                    <pin name="GND39"/>
                    <pin name="GND40"/>
                    <pin name="GND41"/>
                    <pin name="GND42"/>
                    <pin name="GND43"/>
                    <pin name="GND44"/>
                    <pin name="GND45"/>
                    <pin name="GND46"/>
                    <pin name="GND47"/>
                    <pin name="GND48"/>
                    <pin name="GND49"/>
                    <pin name="GND50"/>
                    <pin name="GND51"/>
                    <pin name="GND52"/>
                    <pin name="GND53"/>
                    <pin name="GND54"/>
                </symbol>
                <symbol name="SAMSUNG_SIP-007AFS001_0_2">
                    <description></description>
                    <pin name="AP_MIPICSI_DNCLK"/>
                    <pin name="AP_MIPICSI_DN0"/>
                    <pin name="AP_MIPICSI_DN1"/>
                    <pin name="AP_MIPICSI_DN2"/>
                    <pin name="AP_MIPICSI_DN3"/>
                    <pin name="AP_MIPIDSI_DNCLK"/>
                    <pin name="AP_MIPIDSI_DN0"/>
                    <pin name="AP_MIPIDSI_DN1"/>
                    <pin name="AP_MIPIDSI_DN2"/>
                    <pin name="AP_MIPIDSI_DN3"/>
                    <pin name="AP_MIPICSI_DPCLK"/>
                    <pin name="AP_MIPICSI_DP0"/>
                    <pin name="AP_MIPICSI_DP1"/>
                    <pin name="AP_MIPICSI_DP2"/>
                    <pin name="AP_MIPICSI_DP3"/>
                    <pin name="AP_MIPIDSI_DPCLK"/>
                    <pin name="AP_MIPIDSI_DP0"/>
                    <pin name="AP_MIPIDSI_DP1"/>
                    <pin name="AP_MIPIDSI_DP2"/>
                    <pin name="AP_MIPIDSI_DP3"/>
                    <pin name="AP_DISD6_BOOT"/>
                    <pin name="AP_ADC4"/>
                    <pin name="AP_ADC5"/>
                    <pin name="AP_ADC0"/>
                    <pin name="AP_ADC1"/>
                    <pin name="AP_ADC2"/>
                    <pin name="AP_ADC3"/>
                    <pin name="BT_PCM_D_OUT"/>
                    <pin name="BT_PCM_LRCK"/>
                    <pin name="AP_GPB13_SD0_BOOT"/>
                    <pin name="BT_PCM_D_IN"/>
                    <pin name="AP_GPB4_VID1_3_BOOT"/>
                    <pin name="AP_GPB15_SD1_BOOT"/>
                    <pin name="BT_PCM_CLK"/>
                </symbol>
                <symbol name="SAMSUNG_SIP-007AFS001_0_3">
                    <description></description>
                    <pin name="AP_HDMI_CEC"/>
                    <pin name="AP_HDMI_TX2N"/>
                    <pin name="AP_HDMI_TX1N"/>
                    <pin name="AP_HDMI_TX0N"/>
                    <pin name="AP_HDMI_TXCN"/>
                    <pin name="AP_HSIC_STROBE"/>
                    <pin name="AP_HDMI_HPD"/>
                    <pin name="AP_HDMI_TX2P"/>
                    <pin name="AP_HDMI_TX1P"/>
                    <pin name="AP_HDMI_TX0P"/>
                    <pin name="AP_HDMI_TXCP"/>
                    <pin name="AP_HSIC_DATA"/>
                    <pin name="AP_GPD6_SCL"/>
                    <pin name="AP_GPD4_SCL1"/>
                    <pin name="AP_GPD2_SCL0"/>
                    <pin name="AP_GPA23_HDMI_I2C_SCL"/>
                    <pin name="AP_GPD7_SDA"/>
                    <pin name="AP_GPD5_SDA1"/>
                    <pin name="AP_GPD3_SDA0"/>
                    <pin name="AP_GPA24_HDMI_I2C_SDA"/>
                    <pin name="AP_TCK"/>
                    <pin name="AP_TMS"/>
                    <pin name="AP_TDO"/>
                    <pin name="AP_TDI"/>
                    <pin name="AP_NTRST"/>
                    <pin name="AP_AGP2_RTC_INT_N"/>
                    <pin name="AP_PWRKEY"/>
                    <pin name="AP_AGP1_HOMEKEY"/>
                    <pin name="AP_NRESET"/>
                    <pin name="AP_GPA25_BACKKEY"/>
                    <pin name="AP_GPA26_VOLUP"/>
                    <pin name="AP_GPA0_MENUKEY"/>
                    <pin name="AP_I2S0_LRCLK"/>
                    <pin name="AP_GPA27_VOLDOWN"/>
                    <pin name="AP_I2S0_DOUT"/>
                    <pin name="AP_I2S0_BCLK"/>
                    <pin name="AP_GPB0_VID1_1_I2SLRCK1"/>
                    <pin name="AP_GPA28_I2SMCLK1"/>
                    <pin name="AP_GPA30_VID1_0_I2SBCLK1"/>
                    <pin name="AP_I2S0_DIN"/>
                    <pin name="AP_I2S0_MCLK"/>
                    <pin name="AP_GPB9_I2SDIN1"/>
                    <pin name="AP_GPB6_VID1_4_I2SDOUT1"/>
                </symbol>
                <symbol name="SAMSUNG_SIP-007AFS001_0_4">
                    <description></description>
                    <pin name="AP_VDDPWRON"/>
                    <pin name="AP_LVDS_TN0"/>
                    <pin name="AP_LVDS_TN1"/>
                    <pin name="AP_LVDS_TN2"/>
                    <pin name="AP_LVDS_TN3"/>
                    <pin name="AP_LVDS_TN4"/>
                    <pin name="AP_LVDS_TNCLK"/>
                    <pin name="AP_LVDS_TPCLK"/>
                    <pin name="AP_NBATTF"/>
                    <pin name="AP_OTG_DM"/>
                    <pin name="AP_OTG_DP"/>
                    <pin name="AP_OTG_ID"/>
                    <pin name="AP_USBH_DM"/>
                    <pin name="AP_USBH_DP"/>
                    <pin name="AP_LVDS_TP0"/>
                    <pin name="AP_LVDS_TP1"/>
                    <pin name="AP_LVDS_TP2"/>
                    <pin name="AP_LVDS_TP3"/>
                    <pin name="AP_LVDS_TP4"/>
                    <pin name="AP_GPC9_SPI2_CLK"/>
                    <pin name="AP_GPC10_SPI2_CS"/>
                    <pin name="AP_GPC11_SPI2_MISO"/>
                    <pin name="AP_GPC12_SPI2_MOSI"/>
                    <pin name="AP_GPC14_PWM2"/>
                    <pin name="AP_SPI0_CLK"/>
                    <pin name="AP_SPI0_CS"/>
                    <pin name="AP_SPI0_MISO"/>
                    <pin name="AP_SPI0_MOSI"/>
                    <pin name="ZB_JTCK"/>
                    <pin name="ZB_JTDI"/>
                    <pin name="ZB_JTDO"/>
                    <pin name="ZB_JTMS"/>
                    <pin name="ZB_RSTN"/>
                    <pin name="ZB_PC0"/>
                    <pin name="ZB_PA4"/>
                    <pin name="ZB_PA5"/>
                    <pin name="AP_GPE0"/>
                    <pin name="AP_GPE1"/>
                    <pin name="AP_GPE2"/>
                    <pin name="AP_GPE3"/>
                    <pin name="AP_UARTTX3"/>
                    <pin name="AP_UARTTX4"/>
                    <pin name="AP_UARTTX5"/>
                    <pin name="AP_SD0_CLK"/>
                    <pin name="AP_SD0_CMD"/>
                    <pin name="AP_SD0_D0"/>
                    <pin name="AP_SD0_D1"/>
                    <pin name="AP_SD0_D2"/>
                    <pin name="AP_SD0_D3"/>
                    <pin name="AP_GPB14"/>
                    <pin name="AP_GPB16"/>
                    <pin name="AP_GPD1_PWM0"/>
                    <pin name="AP_GPD31"/>
                    <pin name="AP_UARTRX3"/>
                    <pin name="AP_UARTRX4"/>
                    <pin name="AP_UARTRX5"/>
                </symbol>
                <symbol name="VISHAY_CRCW0805200RFKEA_0_0">
                    <description></description>
                    <pin name="1"/>
                    <pin name="2"/>
                </symbol>
                <symbol name="BOURNS_SRN6045-6R8Y_0_0">
                    <description></description>
                    <pin name="1"/>
                    <pin name="2"/>
                </symbol>
                <symbol name="CTS_218-6LPST_0_0">
                    <description></description>
                    <pin name="1"/>
                    <pin name="6_ON"/>
                    <pin name="2"/>
                    <pin name="5_ON"/>
                    <pin name="3"/>
                    <pin name="4_ON"/>
                    <pin name="4"/>
                    <pin name="3_ON"/>
                    <pin name="5"/>
                    <pin name="2_ON"/>
                    <pin name="6"/>
                    <pin name="1_ON"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_SN74AVC2T244DQMR_0_0">
                    <description></description>
                    <pin name="VCCA"/>
                    <pin name="VCCB"/>
                    <pin name="!OE"/>
                    <pin name="A1"/>
                    <pin name="A2"/>
                    <pin name="B1"/>
                    <pin name="B2"/>
                    <pin name="GND"/>
                </symbol>
                <symbol name="EPSON_FA-20H_16.0000MF12V-AJ3_0_0">
                    <description>MHz Range Crystal Unit</description>
                    <pin name="1"/>
                    <pin name="GND"/>
                    <pin name="3"/>
                    <pin name="GND2"/>
                </symbol>
                <symbol name="SILICON_LABORATORIES_CP2102-GMR_0_0">
                    <description></description>
                    <pin direction="pwr" name="VDD"/>
                    <pin direction="io" name="!RST"/>
                    <pin direction="out" name="!SUSPEND"/>
                    <pin name="CTS"/>
                    <pin direction="io" name="D+"/>
                    <pin direction="io" name="D-"/>
                    <pin direction="in" name="DCD"/>
                    <pin direction="in" name="DSR"/>
                    <pin direction="out" name="DTR"/>
                    <pin direction="in" name="REGIN"/>
                    <pin direction="in" name="RI"/>
                    <pin name="RTS"/>
                    <pin direction="in" name="RXD"/>
                    <pin direction="out" name="SUSPEND"/>
                    <pin direction="out" name="TXD"/>
                    <pin direction="in" name="VBUS"/>
                    <pin name="NC6"/>
                    <pin name="NC"/>
                    <pin name="NC3"/>
                    <pin name="NC4"/>
                    <pin name="NC5"/>
                    <pin name="NC2"/>
                    <pin name="NC10"/>
                    <pin name="NC8"/>
                    <pin name="NC9"/>
                    <pin name="NC11"/>
                    <pin name="NC7"/>
                    <pin name="GND"/>
                    <pin direction="pwr" name="GND_PAD"/>
                </symbol>
                <symbol name="IXYS_CPC1927J_0_0">
                    <description></description>
                    <pin name="1_DRAIN"/>
                    <pin name="2_DRAIN"/>
                    <pin name="CATHODE"/>
                    <pin name="ANODE"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_BQ294700DSGR_0_0">
                    <description></description>
                    <pin direction="pwr" name="VDD"/>
                    <pin direction="out" name="CD"/>
                    <pin direction="out" name="OUT"/>
                    <pin direction="in" name="V1"/>
                    <pin direction="in" name="V2"/>
                    <pin direction="in" name="V3"/>
                    <pin direction="in" name="V4"/>
                    <pin direction="pwr" name="GND_PAD"/>
                    <pin direction="pwr" name="VSS"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_BQ24259RGER_0_0">
                    <description></description>
                    <pin name="VBUS"/>
                    <pin name="VBUS2"/>
                    <pin name="BAT"/>
                    <pin name="BAT2"/>
                    <pin name="SYS"/>
                    <pin name="SYS2"/>
                    <pin name="SW"/>
                    <pin name="SW2"/>
                    <pin name="!CE"/>
                    <pin name="!PG"/>
                    <pin name="BTST"/>
                    <pin name="ILIM"/>
                    <pin name="INT"/>
                    <pin name="OTG"/>
                    <pin name="PMID"/>
                    <pin name="PSEL"/>
                    <pin name="QON"/>
                    <pin name="REGN"/>
                    <pin name="SCL"/>
                    <pin name="SDA"/>
                    <pin name="STAT"/>
                    <pin name="TS"/>
                    <pin name="THERMAL_PAD"/>
                    <pin name="PGND"/>
                    <pin name="PGND2"/>
                </symbol>
                <symbol name="BOURNS_PEC16-4220F-S0024_0_0">
                    <description></description>
                    <pin name="MNT_1"/>
                    <pin name="MNT_2"/>
                    <pin name="A"/>
                    <pin name="B"/>
                    <pin name="C"/>
                    <pin name="D"/>
                    <pin name="E"/>
                </symbol>
                <symbol name="AVX_F950J476MPAAQ2_0_0">
                    <description></description>
                    <pin name="CATHODE"/>
                    <pin name="ANODE"/>
                </symbol>
                <symbol name="PANASONIC_ERJ-3EKF22R0V_0_0">
                    <description></description>
                    <pin name="1"/>
                    <pin name="2"/>
                </symbol>
                <symbol name="ST_MICROELECTRONICS_L7805CDT-TR_0_0">
                    <description></description>
                    <pin direction="in" name="IN"/>
                    <pin direction="out" name="OUT"/>
                    <pin direction="pwr" name="GND"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_TLC5955RTQR_0_0">
                    <description></description>
                    <pin name="OUTB3"/>
                    <pin name="OUTR3"/>
                    <pin name="OUTG3"/>
                    <pin name="OUTB7"/>
                    <pin name="OUTR7"/>
                    <pin name="OUTG7"/>
                    <pin name="SOUT"/>
                    <pin name="GND"/>
                    <pin name="OUTG11"/>
                    <pin name="OUTR11"/>
                    <pin name="OUTB11"/>
                    <pin name="OUTG15"/>
                    <pin name="OUTR15"/>
                    <pin name="OUTB15"/>
                    <pin name="OUTG10"/>
                    <pin name="OUTR10"/>
                    <pin name="OUTB10"/>
                    <pin name="OUTG14"/>
                    <pin name="OUTR14"/>
                    <pin name="OUTB14"/>
                    <pin name="OUTG13"/>
                    <pin name="OUTR13"/>
                    <pin name="OUTB13"/>
                    <pin name="OUTG9"/>
                    <pin name="OUTR9"/>
                    <pin name="OUTB9"/>
                    <pin name="OUTG12"/>
                    <pin name="OUTR12"/>
                    <pin name="OUTB12"/>
                    <pin name="OUTG8"/>
                    <pin name="OUTR8"/>
                    <pin name="OUTB8"/>
                    <pin name="VCC"/>
                    <pin name="GSCLK"/>
                    <pin name="GND2"/>
                    <pin name="SIN"/>
                    <pin name="SCLK"/>
                    <pin name="LAT"/>
                    <pin name="OUTB4"/>
                    <pin name="OUTR4"/>
                    <pin name="OUTG4"/>
                    <pin name="OUTB0"/>
                    <pin name="OUTR0"/>
                    <pin name="OUTG0"/>
                    <pin name="OUTB5"/>
                    <pin name="OUTR5"/>
                    <pin name="OUTG5"/>
                    <pin name="OUTB1"/>
                    <pin name="OUTR1"/>
                    <pin name="OUTG1"/>
                    <pin name="OUTB2"/>
                    <pin name="OUTR2"/>
                    <pin name="OUTG2"/>
                    <pin name="OUTB6"/>
                    <pin name="OUTR6"/>
                    <pin name="OUTG6"/>
                    <pin name="GND_PAD"/>
                </symbol>
                <symbol name="DIODES_MMSZ5233B_0_0">
                    <description></description>
                    <pin name="ANODE"/>
                    <pin name="CATHODE"/>
                </symbol>
                <symbol name="E-SWITCH_TL1015AF160QG_0_0">
                    <description></description>
                    <pin name="1"/>
                    <pin name="2"/>
                    <pin name="G"/>
                    <pin name="G2"/>
                    <pin name="G3"/>
                    <pin name="G4"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_0">
                    <description></description>
                    <pin name="CAP_VDD_RTC"/>
                    <pin name="CAP_VDD_SRAM_CORE"/>
                    <pin name="CAP_VDD_SRAM_MPU"/>
                    <pin name="CAP_VDDS1P8V_IOLDO"/>
                    <pin name="VDDA1P8V_USB0"/>
                    <pin name="VDDA1P8V_USB1"/>
                    <pin name="VDDA3P3V_USB0"/>
                    <pin name="VDDA3P3V_USB1"/>
                    <pin name="VDDA_ADC0"/>
                    <pin name="VDDA_ADC1"/>
                    <pin name="CAP_VBB_MPU"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_1">
                    <description></description>
                    <pin name="EMU0"/>
                    <pin name="EMU1"/>
                    <pin name="GPIO5_8"/>
                    <pin name="GPIO5_9"/>
                    <pin name="GPIO5_10"/>
                    <pin name="GPIO5_11"/>
                    <pin name="GPIO5_12"/>
                    <pin name="GPIO5_13"/>
                    <pin name="I2C0_SCL"/>
                    <pin name="I2C0_SDA"/>
                    <pin name="MCASP0_ACLKR"/>
                    <pin name="MCASP0_ACLKX"/>
                    <pin name="MCASP0_AHCLKR"/>
                    <pin name="MCASP0_AHCLKX"/>
                    <pin name="MCASP0_AXR0"/>
                    <pin name="MCASP0_AXR1"/>
                    <pin name="MCASP0_FSR"/>
                    <pin name="MCASP0_FSX"/>
                    <pin name="UART0_CTSN"/>
                    <pin name="UART0_RTSN"/>
                    <pin name="UART0_RXD"/>
                    <pin name="UART0_TXD"/>
                    <pin name="UART1_CTSN"/>
                    <pin name="UART1_RTSN"/>
                    <pin name="UART1_RXD"/>
                    <pin name="UART1_TXD"/>
                    <pin name="UART3_CTSN"/>
                    <pin name="UART3_RTSN"/>
                    <pin name="UART3_RXD"/>
                    <pin name="UART3_TXD"/>
                    <pin name="CLKREQ"/>
                    <pin name="ECAP0_IN_PWM0_OUT"/>
                    <pin name="EXTINTN"/>
                    <pin name="NTRST"/>
                    <pin name="PWRONRSTN"/>
                    <pin name="SPI0_CS0"/>
                    <pin name="WARMRSTN"/>
                    <pin name="USB0_DRVVBUS"/>
                    <pin name="USB1_DRVVBUS"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_2">
                    <description></description>
                    <pin name="DDR_BA0"/>
                    <pin name="DDR_BA1"/>
                    <pin name="DDR_BA2"/>
                    <pin name="DDR_CASN"/>
                    <pin name="DDR_CK"/>
                    <pin name="DDR_NCK"/>
                    <pin name="DDR_RASN"/>
                    <pin name="DDR_RESETN"/>
                    <pin name="DDR_VREF"/>
                    <pin name="DDR_VTP"/>
                    <pin name="DDR_WEN"/>
                    <pin name="DDR_CKE0"/>
                    <pin name="DDR_CKE1"/>
                    <pin name="DDR_CSN0"/>
                    <pin name="DDR_CSN1"/>
                    <pin name="DDR_DQM0"/>
                    <pin name="DDR_DQM1"/>
                    <pin name="DDR_DQM2"/>
                    <pin name="DDR_DQM3"/>
                    <pin name="DDR_DQS0"/>
                    <pin name="DDR_DQS1"/>
                    <pin name="DDR_DQS2"/>
                    <pin name="DDR_DQS3"/>
                    <pin name="DDR_DQSN0"/>
                    <pin name="DDR_DQSN1"/>
                    <pin name="DDR_DQSN2"/>
                    <pin name="DDR_DQSN3"/>
                    <pin name="DDR_ODT0"/>
                    <pin name="DDR_ODT1"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_3">
                    <description></description>
                    <pin name="GPMC_A0"/>
                    <pin name="GPMC_A1"/>
                    <pin name="GPMC_A2"/>
                    <pin name="GPMC_A3"/>
                    <pin name="GPMC_A4"/>
                    <pin name="GPMC_A5"/>
                    <pin name="GPMC_A6"/>
                    <pin name="GPMC_A7"/>
                    <pin name="GPMC_A8"/>
                    <pin name="GPMC_A9"/>
                    <pin name="GPMC_A10"/>
                    <pin name="GPMC_A11"/>
                    <pin name="GPMC_BE1N"/>
                    <pin name="GPMC_WAIT0"/>
                    <pin name="GPMC_WPN"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_4">
                    <description></description>
                    <pin name="CAM0_DATA0"/>
                    <pin name="CAM0_DATA1"/>
                    <pin name="CAM0_DATA2"/>
                    <pin name="CAM0_DATA3"/>
                    <pin name="CAM0_DATA4"/>
                    <pin name="CAM0_DATA5"/>
                    <pin name="CAM0_DATA6"/>
                    <pin name="CAM0_DATA7"/>
                    <pin name="CAM0_DATA8"/>
                    <pin name="CAM0_DATA9"/>
                    <pin name="CAM0_FIELD"/>
                    <pin name="CAM0_HD"/>
                    <pin name="CAM0_PCLK"/>
                    <pin name="CAM0_VD"/>
                    <pin name="CAM0_WEN"/>
                    <pin name="CAM1_DATA0"/>
                    <pin name="CAM1_DATA1"/>
                    <pin name="CAM1_DATA2"/>
                    <pin name="CAM1_DATA3"/>
                    <pin name="CAM1_DATA4"/>
                    <pin name="CAM1_DATA5"/>
                    <pin name="CAM1_DATA6"/>
                    <pin name="CAM1_DATA7"/>
                    <pin name="CAM1_DATA8"/>
                    <pin name="CAM1_DATA9"/>
                    <pin name="CAM1_FIELD"/>
                    <pin name="CAM1_HD"/>
                    <pin name="CAM1_PCLK"/>
                    <pin name="CAM1_VD"/>
                    <pin name="CAM1_WEN"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_5">
                    <description></description>
                    <pin name="DSS_AC_BIAS_EN"/>
                    <pin name="DSS_HSYNC"/>
                    <pin name="DSS_PCLK"/>
                    <pin name="DSS_VSYNC"/>
                    <pin name="DSS_DATA0"/>
                    <pin name="DSS_DATA1"/>
                    <pin name="DSS_DATA2"/>
                    <pin name="DSS_DATA3"/>
                    <pin name="DSS_DATA4"/>
                    <pin name="DSS_DATA5"/>
                    <pin name="DSS_DATA6"/>
                    <pin name="DSS_DATA7"/>
                    <pin name="DSS_DATA8"/>
                    <pin name="DSS_DATA9"/>
                    <pin name="DSS_DATA10"/>
                    <pin name="DSS_DATA11"/>
                    <pin name="DSS_DATA12"/>
                    <pin name="DSS_DATA13"/>
                    <pin name="DSS_DATA14"/>
                    <pin name="DSS_DATA15"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_6">
                    <description></description>
                    <pin name="SPI0_CS1"/>
                    <pin name="SPI0_D0"/>
                    <pin name="SPI0_D1"/>
                    <pin name="SPI0_SCLK"/>
                    <pin name="SPI2_CS0"/>
                    <pin name="SPI2_D0"/>
                    <pin name="SPI2_D1"/>
                    <pin name="SPI2_SCLK"/>
                    <pin name="SPI4_CS0"/>
                    <pin name="SPI4_D0"/>
                    <pin name="SPI4_D1"/>
                    <pin name="SPI4_SCLK"/>
                    <pin name="TCK"/>
                    <pin name="TDI"/>
                    <pin name="TDO"/>
                    <pin name="TMS"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_7">
                    <description></description>
                    <pin name="MII1_COL"/>
                    <pin name="MII1_CRS"/>
                    <pin name="MII1_RX_CLK"/>
                    <pin name="MII1_RX_DV"/>
                    <pin name="MII1_RX_ER"/>
                    <pin name="MII1_RXD0"/>
                    <pin name="MII1_RXD1"/>
                    <pin name="MII1_RXD2"/>
                    <pin name="MII1_RXD3"/>
                    <pin name="MII1_TX_CLK"/>
                    <pin name="MII1_TX_EN"/>
                    <pin name="MII1_TXD0"/>
                    <pin name="MII1_TXD1"/>
                    <pin name="MII1_TXD2"/>
                    <pin name="MII1_TXD3"/>
                    <pin name="RMII1_REF_CLK"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_8">
                    <description></description>
                    <pin name="VSS4"/>
                    <pin name="VSS69"/>
                    <pin name="VSS54"/>
                    <pin name="VSS8"/>
                    <pin name="VSS7"/>
                    <pin name="VSS39"/>
                    <pin name="VSS68"/>
                    <pin name="VSS67"/>
                    <pin name="VSS66"/>
                    <pin name="VSS23"/>
                    <pin name="VSS52"/>
                    <pin name="VSS57"/>
                    <pin name="VSS58"/>
                    <pin name="VSS53"/>
                    <pin name="VSS10"/>
                    <pin name="VSS11"/>
                    <pin name="VSS43"/>
                    <pin name="VSS41"/>
                    <pin name="VSS42"/>
                    <pin name="VSS40"/>
                    <pin name="VSS28"/>
                    <pin name="VSS27"/>
                    <pin name="VSS29"/>
                    <pin name="VSS30"/>
                    <pin name="VSS31"/>
                    <pin name="VSS17"/>
                    <pin name="VSS18"/>
                    <pin name="VSS15"/>
                    <pin name="VSS16"/>
                    <pin name="VSS19"/>
                    <pin name="VSS20"/>
                    <pin name="VSS47"/>
                    <pin name="VSS48"/>
                    <pin name="VSS"/>
                    <pin name="VSS2"/>
                    <pin name="VSS3"/>
                    <pin name="VSS55"/>
                    <pin name="VSS5"/>
                    <pin name="VSS6"/>
                    <pin name="VSS64"/>
                    <pin name="VSS63"/>
                    <pin name="VSS62"/>
                    <pin name="VSS65"/>
                    <pin name="VSS46"/>
                    <pin name="VSS44"/>
                    <pin name="VSS45"/>
                    <pin name="VSS60"/>
                    <pin name="VSS59"/>
                    <pin name="VSS22"/>
                    <pin name="VSS21"/>
                    <pin name="VSS14"/>
                    <pin name="VSS13"/>
                    <pin name="VSS24"/>
                    <pin name="VSS26"/>
                    <pin name="VSS25"/>
                    <pin name="VSS32"/>
                    <pin name="VSS12"/>
                    <pin name="VSS56"/>
                    <pin name="VSS36"/>
                    <pin name="VSS37"/>
                    <pin name="VSS34"/>
                    <pin name="VSS35"/>
                    <pin name="VSS38"/>
                    <pin name="VSS33"/>
                    <pin name="VSS51"/>
                    <pin name="VSS9"/>
                    <pin name="VSS50"/>
                    <pin name="VSS49"/>
                    <pin name="VSS61"/>
                    <pin name="VSS_OSC"/>
                    <pin name="VSS_RTC"/>
                    <pin name="VSSA_ADC"/>
                    <pin name="VSSA_USB"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_9">
                    <description></description>
                    <pin name="RESERVED25"/>
                    <pin name="RESERVED2"/>
                    <pin name="RESERVED9"/>
                    <pin name="RESERVED8"/>
                    <pin name="RESERVED7"/>
                    <pin name="RESERVED6"/>
                    <pin name="RESERVED"/>
                    <pin name="RESERVED11"/>
                    <pin name="RESERVED28"/>
                    <pin name="RESERVED27"/>
                    <pin name="RESERVED3"/>
                    <pin name="RESERVED4"/>
                    <pin name="RESERVED5"/>
                    <pin name="RESERVED17"/>
                    <pin name="RESERVED10"/>
                    <pin name="RESERVED24"/>
                    <pin name="RESERVED23"/>
                    <pin name="RESERVED26"/>
                    <pin name="RESERVED13"/>
                    <pin name="RESERVED12"/>
                    <pin name="RESERVED22"/>
                    <pin name="RESERVED21"/>
                    <pin name="RESERVED20"/>
                    <pin name="RESERVED18"/>
                    <pin name="RESERVED19"/>
                    <pin name="RESERVED14"/>
                    <pin name="RESERVED15"/>
                    <pin name="RESERVED16"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_10">
                    <description></description>
                    <pin name="VDD_MPU10"/>
                    <pin name="VDD_MPU5"/>
                    <pin name="VDD_MPU2"/>
                    <pin name="VDD_MPU3"/>
                    <pin name="VDD_MPU12"/>
                    <pin name="VDD_MPU11"/>
                    <pin name="VDD_MPU"/>
                    <pin name="VDD_MPU8"/>
                    <pin name="VDD_MPU6"/>
                    <pin name="VDD_MPU7"/>
                    <pin name="VDD_MPU9"/>
                    <pin name="VDD_MPU4"/>
                    <pin name="VDD_MPU_MON"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_11">
                    <description></description>
                    <pin name="VDDS7"/>
                    <pin name="VDDS8"/>
                    <pin name="VDDS2"/>
                    <pin name="VDDS6"/>
                    <pin name="VDDS5"/>
                    <pin name="VDDS"/>
                    <pin name="VDDS4"/>
                    <pin name="VDDS3"/>
                    <pin name="VDDS3P3V_IOLDO"/>
                    <pin name="VDDS_CLKOUT"/>
                    <pin name="VDDS_DDR6"/>
                    <pin name="VDDS_DDR7"/>
                    <pin name="VDDS_DDR"/>
                    <pin name="VDDS_DDR2"/>
                    <pin name="VDDS_DDR11"/>
                    <pin name="VDDS_DDR9"/>
                    <pin name="VDDS_DDR8"/>
                    <pin name="VDDS_DDR10"/>
                    <pin name="VDDS_DDR3"/>
                    <pin name="VDDS_DDR4"/>
                    <pin name="VDDS_DDR5"/>
                    <pin name="VDDS_DDR13"/>
                    <pin name="VDDS_DDR12"/>
                    <pin name="VDDS_OSC"/>
                    <pin name="VDDS_PLL_CORE_LCD"/>
                    <pin name="VDDS_PLL_DDR"/>
                    <pin name="VDDS_PLL_MPU"/>
                    <pin name="VDDS_RTC"/>
                    <pin name="VDDS_SRAM_CORE_BG"/>
                    <pin name="VDDS_SRAM_MPU_BB"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_12">
                    <description></description>
                    <pin name="VDDSHV1"/>
                    <pin name="VDDSHV12"/>
                    <pin name="VDDSHV23"/>
                    <pin name="VDDSHV22"/>
                    <pin name="VDDSHV2"/>
                    <pin name="VDDSHV33"/>
                    <pin name="VDDSHV32"/>
                    <pin name="VDDSHV35"/>
                    <pin name="VDDSHV36"/>
                    <pin name="VDDSHV3"/>
                    <pin name="VDDSHV34"/>
                    <pin name="VDDSHV37"/>
                    <pin name="VDDSHV5"/>
                    <pin name="VDDSHV62"/>
                    <pin name="VDDSHV6"/>
                    <pin name="VDDSHV63"/>
                    <pin name="VDDSHV7"/>
                    <pin name="VDDSHV8"/>
                    <pin name="VDDSHV82"/>
                    <pin name="VDDSHV92"/>
                    <pin name="VDDSHV9"/>
                    <pin name="VDDSHV102"/>
                    <pin name="VDDSHV10"/>
                    <pin name="VDDSHV11"/>
                    <pin name="VDDSHV112"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_13">
                    <description></description>
                    <pin name="DDR_D0"/>
                    <pin name="DDR_D1"/>
                    <pin name="DDR_D2"/>
                    <pin name="DDR_D3"/>
                    <pin name="DDR_D4"/>
                    <pin name="DDR_D5"/>
                    <pin name="DDR_D6"/>
                    <pin name="DDR_D7"/>
                    <pin name="DDR_D8"/>
                    <pin name="DDR_D9"/>
                    <pin name="DDR_D10"/>
                    <pin name="DDR_D11"/>
                    <pin name="DDR_D12"/>
                    <pin name="DDR_D13"/>
                    <pin name="DDR_D14"/>
                    <pin name="DDR_D15"/>
                    <pin name="DDR_D16"/>
                    <pin name="DDR_D17"/>
                    <pin name="DDR_D18"/>
                    <pin name="DDR_D19"/>
                    <pin name="DDR_D20"/>
                    <pin name="DDR_D21"/>
                    <pin name="DDR_D22"/>
                    <pin name="DDR_D23"/>
                    <pin name="DDR_D24"/>
                    <pin name="DDR_D25"/>
                    <pin name="DDR_D26"/>
                    <pin name="DDR_D27"/>
                    <pin name="DDR_D28"/>
                    <pin name="DDR_D29"/>
                    <pin name="DDR_D30"/>
                    <pin name="DDR_D31"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_14">
                    <description></description>
                    <pin name="DDR_A0"/>
                    <pin name="DDR_A1"/>
                    <pin name="DDR_A2"/>
                    <pin name="DDR_A3"/>
                    <pin name="DDR_A4"/>
                    <pin name="DDR_A5"/>
                    <pin name="DDR_A6"/>
                    <pin name="DDR_A7"/>
                    <pin name="DDR_A8"/>
                    <pin name="DDR_A9"/>
                    <pin name="DDR_A10"/>
                    <pin name="DDR_A11"/>
                    <pin name="DDR_A12"/>
                    <pin name="DDR_A13"/>
                    <pin name="DDR_A14"/>
                    <pin name="DDR_A15"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_15">
                    <description></description>
                    <pin name="VDD_CORE4"/>
                    <pin name="VDD_CORE22"/>
                    <pin name="VDD_CORE14"/>
                    <pin name="VDD_CORE13"/>
                    <pin name="VDD_CORE"/>
                    <pin name="VDD_CORE10"/>
                    <pin name="VDD_CORE11"/>
                    <pin name="VDD_CORE24"/>
                    <pin name="VDD_CORE7"/>
                    <pin name="VDD_CORE8"/>
                    <pin name="VDD_CORE2"/>
                    <pin name="VDD_CORE3"/>
                    <pin name="VDD_CORE23"/>
                    <pin name="VDD_CORE20"/>
                    <pin name="VDD_CORE19"/>
                    <pin name="VDD_CORE25"/>
                    <pin name="VDD_CORE16"/>
                    <pin name="VDD_CORE15"/>
                    <pin name="VDD_CORE17"/>
                    <pin name="VDD_CORE18"/>
                    <pin name="VDD_CORE9"/>
                    <pin name="VDD_CORE12"/>
                    <pin name="VDD_CORE6"/>
                    <pin name="VDD_CORE5"/>
                    <pin name="VDD_CORE21"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_16">
                    <description></description>
                    <pin name="MDIO_CLK"/>
                    <pin name="MDIO_DATA"/>
                    <pin name="XDMA_EVENT_INTR0"/>
                    <pin name="XDMA_EVENT_INTR1"/>
                    <pin name="XTALIN"/>
                    <pin name="XTALOUT"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_17">
                    <description></description>
                    <pin name="ADC0_AIN0"/>
                    <pin name="ADC0_AIN1"/>
                    <pin name="ADC0_AIN2"/>
                    <pin name="ADC0_AIN3"/>
                    <pin name="ADC0_AIN4"/>
                    <pin name="ADC0_AIN5"/>
                    <pin name="ADC0_AIN6"/>
                    <pin name="ADC0_AIN7"/>
                    <pin name="ADC0_VREFN"/>
                    <pin name="ADC0_VREFP"/>
                    <pin name="ADC1_AIN0"/>
                    <pin name="ADC1_AIN1"/>
                    <pin name="ADC1_AIN2"/>
                    <pin name="ADC1_AIN3"/>
                    <pin name="ADC1_AIN4"/>
                    <pin name="ADC1_AIN5"/>
                    <pin name="ADC1_AIN6"/>
                    <pin name="ADC1_AIN7"/>
                    <pin name="ADC1_VREFN"/>
                    <pin name="ADC1_VREFP"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_18">
                    <description></description>
                    <pin name="USB0_CE"/>
                    <pin name="USB0_DM"/>
                    <pin name="USB0_DP"/>
                    <pin name="USB0_ID"/>
                    <pin name="USB0_VBUS"/>
                    <pin name="USB1_CE"/>
                    <pin name="USB1_DM"/>
                    <pin name="USB1_DP"/>
                    <pin name="USB1_ID"/>
                    <pin name="USB1_VBUS"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_19">
                    <description></description>
                    <pin name="GPMC_AD0"/>
                    <pin name="GPMC_AD1"/>
                    <pin name="GPMC_AD2"/>
                    <pin name="GPMC_AD3"/>
                    <pin name="GPMC_AD4"/>
                    <pin name="GPMC_AD5"/>
                    <pin name="GPMC_AD6"/>
                    <pin name="GPMC_AD7"/>
                    <pin name="GPMC_AD8"/>
                    <pin name="GPMC_AD9"/>
                    <pin name="GPMC_AD10"/>
                    <pin name="GPMC_AD11"/>
                    <pin name="GPMC_AD12"/>
                    <pin name="GPMC_AD13"/>
                    <pin name="GPMC_AD14"/>
                    <pin name="GPMC_AD15"/>
                    <pin name="GPMC_BE0N_CLE"/>
                    <pin name="GPMC_CSN0"/>
                    <pin name="GPMC_CSN1"/>
                    <pin name="GPMC_CSN2"/>
                    <pin name="GPMC_CSN3"/>
                    <pin name="GPMC_ADVN_ALE"/>
                    <pin name="GPMC_CLK"/>
                    <pin name="GPMC_OEN_REN"/>
                    <pin name="GPMC_WEN"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_20">
                    <description></description>
                    <pin name="MMC0_CLK"/>
                    <pin name="MMC0_CMD"/>
                    <pin name="MMC0_DAT0"/>
                    <pin name="MMC0_DAT1"/>
                    <pin name="MMC0_DAT2"/>
                    <pin name="MMC0_DAT3"/>
                    <pin name="RTC_KALDO_ENN"/>
                    <pin name="RTC_PMIC_EN"/>
                    <pin name="RTC_PWRONRSTN"/>
                    <pin name="RTC_WAKEUP"/>
                    <pin name="RTC_XTALIN"/>
                    <pin name="RTC_XTALOUT"/>
                </symbol>
                <symbol name="ANALOG_DEVICES_INC._ADV7180BSTZ_0_0">
                    <description></description>
                    <pin direction="in" name="!PWRDWN"/>
                    <pin direction="in" name="!RESET"/>
                    <pin direction="in" name="AIN1"/>
                    <pin direction="in" name="AIN2"/>
                    <pin direction="in" name="AIN3"/>
                    <pin direction="in" name="AIN4"/>
                    <pin direction="in" name="AIN5"/>
                    <pin direction="in" name="AIN6"/>
                    <pin direction="in" name="ALSB"/>
                    <pin direction="in" name="SCLK"/>
                    <pin direction="io" name="SDATA"/>
                    <pin direction="in" name="TEST_0"/>
                    <pin direction="out" name="VREFN"/>
                    <pin direction="out" name="VREFP"/>
                    <pin direction="in" name="XTAL"/>
                    <pin direction="out" name="XTAL1"/>
                    <pin direction="out" name="!INTRQ"/>
                    <pin direction="in" name="ELPF"/>
                    <pin direction="out" name="FIELD"/>
                    <pin direction="out" name="GPO2"/>
                    <pin direction="out" name="GPO3"/>
                    <pin direction="out" name="GPO0"/>
                    <pin direction="out" name="GPO1"/>
                    <pin direction="out" name="HS"/>
                    <pin direction="out" name="LLC"/>
                    <pin direction="out" name="P0"/>
                    <pin direction="out" name="P1"/>
                    <pin direction="out" name="P2"/>
                    <pin direction="out" name="P3"/>
                    <pin direction="out" name="P4"/>
                    <pin direction="out" name="P5"/>
                    <pin direction="out" name="P6"/>
                    <pin direction="out" name="P7"/>
                    <pin direction="out" name="P8"/>
                    <pin direction="out" name="P9"/>
                    <pin direction="out" name="P10"/>
                    <pin direction="out" name="P11"/>
                    <pin direction="out" name="P12"/>
                    <pin direction="out" name="P13"/>
                    <pin direction="out" name="P14"/>
                    <pin direction="out" name="P15"/>
                    <pin direction="out" name="SFL"/>
                    <pin direction="out" name="VS"/>
                </symbol>
                <symbol name="ANALOG_DEVICES_INC._ADV7180BSTZ_0_1">
                    <description></description>
                    <pin direction="pwr" name="AVDD"/>
                    <pin direction="pwr" name="DVDD"/>
                    <pin direction="pwr" name="DVDD2"/>
                    <pin name="DVDDIO2"/>
                    <pin direction="pwr" name="DVDDIO"/>
                    <pin name="NC5"/>
                    <pin name="NC6"/>
                    <pin name="NC7"/>
                    <pin name="NC4"/>
                    <pin name="NC"/>
                    <pin name="NC2"/>
                    <pin name="NC8"/>
                    <pin name="NC3"/>
                    <pin direction="pwr" name="PVDD"/>
                    <pin direction="pwr" name="AGND2"/>
                    <pin direction="pwr" name="AGND"/>
                    <pin direction="pwr" name="AGND3"/>
                    <pin direction="pwr" name="DGND3"/>
                    <pin direction="pwr" name="DGND"/>
                    <pin direction="pwr" name="DGND4"/>
                    <pin name="DGND2"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_TPS65218B1RSLT_0_0">
                    <description></description>
                    <pin direction="pwr" name="CC"/>
                    <pin direction="pwr" name="DCDC4"/>
                    <pin direction="pwr" name="INT_LDO"/>
                    <pin direction="pwr" name="IN_BIAS"/>
                    <pin direction="pwr" name="IN_BU"/>
                    <pin direction="pwr" name="IN_DCDC2"/>
                    <pin direction="pwr" name="IN_DCDC3"/>
                    <pin direction="pwr" name="IN_DCDC4"/>
                    <pin direction="pwr" name="IN_LD01"/>
                    <pin direction="pwr" name="IN_LS1"/>
                    <pin direction="pwr" name="IN_LS3"/>
                    <pin direction="pwr" name="L1"/>
                    <pin direction="pwr" name="L2"/>
                    <pin direction="pwr" name="L3"/>
                    <pin direction="pwr" name="L4A"/>
                    <pin direction="pwr" name="L4B"/>
                    <pin direction="pwr" name="L5"/>
                    <pin direction="pwr" name="L6"/>
                    <pin direction="pwr" name="SYS_BU"/>
                    <pin name="NC"/>
                    <pin name="NC2"/>
                    <pin direction="pwr" name="GND_PAD"/>
                    <pin direction="pwr" name="IN_DCDC1"/>
                    <pin direction="io" name="SDA"/>
                    <pin direction="in" name="SCL"/>
                    <pin direction="in" name="PFI"/>
                    <pin direction="in" name="DC34_SEL"/>
                    <pin direction="in" name="FB5"/>
                    <pin direction="in" name="FB6"/>
                    <pin direction="in" name="FB3"/>
                    <pin direction="in" name="FB2"/>
                    <pin direction="in" name="PB"/>
                    <pin direction="in" name="PWR_EN"/>
                    <pin direction="in" name="FB1"/>
                    <pin direction="in" name="IN_LS2"/>
                    <pin direction="out" name="LS2"/>
                    <pin direction="out" name="LD01"/>
                    <pin direction="out" name="LS3"/>
                    <pin direction="out" name="IN_NCC"/>
                    <pin direction="out" name="PGOOD_BU"/>
                    <pin direction="out" name="LS1"/>
                    <pin direction="io" name="GPIO1"/>
                    <pin direction="io" name="GPIO3"/>
                    <pin direction="out" name="GPO2"/>
                    <pin direction="in" name="AC_DET"/>
                    <pin direction="out" name="PGOOD"/>
                    <pin direction="out" name="!PFO"/>
                    <pin direction="out" name="!WAKEUP"/>
                    <pin direction="out" name="!INT"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_TPS62160DSGR_0_0">
                    <description></description>
                    <pin direction="pwr" name="VIN"/>
                    <pin direction="in" name="EN"/>
                    <pin direction="in" name="FB"/>
                    <pin direction="out" name="PG"/>
                    <pin direction="out" name="SW"/>
                    <pin direction="in" name="VOS"/>
                    <pin direction="pwr" name="AGND"/>
                    <pin direction="pwr" name="AGND_PAD"/>
                    <pin direction="pwr" name="PGND"/>
                </symbol>
                <symbol name="JST_SM02B-SRSS-TB_LF_SN_0_0">
                    <description></description>
                    <pin name="1"/>
                    <pin name="2"/>
                    <pin name="MNT_1"/>
                    <pin name="MNT_2"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_LMP7702MA_0_0">
                    <description></description>
                    <pin direction="in" name="IN_A+"/>
                    <pin direction="in" name="IN_A–"/>
                    <pin direction="out" name="OUT_A"/>
                    <pin direction="pwr" name="V+"/>
                    <pin direction="pwr" name="V–"/>
                </symbol>
                <symbol name="TEXAS_INSTRUMENTS_LMP7702MA_0_1">
                    <description></description>
                    <pin direction="in" name="IN_B+"/>
                    <pin direction="in" name="IN_B–"/>
                    <pin direction="out" name="OUT_B"/>
                </symbol>
                <symbol name="VISHAY_SIA519EDJ-T1-GE3_0_0">
                    <description>Mosfet Array N and P-Channel 20V 4.5A 7.8W Surface Mount PowerPAK® SC-70-6 Dual</description>
                    <pin name="G1"/>
                    <pin name="S1"/>
                    <pin name="D1"/>
                    <pin name="D12"/>
                </symbol>
                <symbol name="VISHAY_SIA519EDJ-T1-GE3_0_1">
                    <description>Mosfet Array N and P-Channel 20V 4.5A 7.8W Surface Mount PowerPAK® SC-70-6 Dual</description>
                    <pin name="G2"/>
                    <pin name="S2"/>
                    <pin name="D2"/>
                    <pin name="D22"/>
                </symbol>
                <symbol name="MICRON_TECHNOLOGY_INC._MT29F256G08CMCABH2-12Z_0_0">
                    <description></description>
                    <pin direction="pas" name="RFU"/>
                    <pin direction="pas" name="RFU2"/>
                    <pin direction="pas" name="RFU3"/>
                    <pin direction="pas" name="RFU4"/>
                    <pin direction="pas" name="RFU5"/>
                    <pin direction="pas" name="RFU6"/>
                    <pin direction="pas" name="RFU7"/>
                    <pin direction="pas" name="RFU8"/>
                    <pin direction="pas" name="RFU9"/>
                    <pin direction="pas" name="RFU10"/>
                    <pin direction="pas" name="DNU"/>
                    <pin direction="pas" name="DNU2"/>
                    <pin direction="pas" name="DNU3"/>
                    <pin direction="pas" name="DNU4"/>
                    <pin direction="pwr" name="VCC"/>
                    <pin direction="pwr" name="VCC2"/>
                    <pin direction="pwr" name="VCC3"/>
                    <pin direction="pwr" name="VCC4"/>
                    <pin direction="pwr" name="VCC5"/>
                    <pin direction="pwr" name="VCC6"/>
                    <pin direction="pwr" name="VCC7"/>
                    <pin direction="pwr" name="VCC8"/>
                    <pin direction="pwr" name="VSS"/>
                    <pin direction="pwr" name="VSS2"/>
                    <pin direction="pwr" name="VSS3"/>
                    <pin direction="pwr" name="VSS4"/>
                    <pin direction="pwr" name="VSS5"/>
                    <pin direction="pwr" name="VSS6"/>
                    <pin direction="pwr" name="VSS7"/>
                    <pin direction="pwr" name="VSS8"/>
                    <pin direction="pwr" name="VSSQ"/>
                    <pin direction="pwr" name="VSSQ2"/>
                    <pin direction="pwr" name="VSSQ3"/>
                    <pin direction="pwr" name="VSSQ4"/>
                    <pin direction="pwr" name="VSSQ5"/>
                    <pin direction="pwr" name="VSSQ6"/>
                    <pin direction="pwr" name="VSSQ7"/>
                    <pin direction="pwr" name="VSSQ8"/>
                    <pin direction="pwr" name="VCCQ"/>
                    <pin direction="pwr" name="VCCQ2"/>
                    <pin direction="pwr" name="VCCQ3"/>
                    <pin direction="pwr" name="VCCQ4"/>
                    <pin direction="pwr" name="VCCQ5"/>
                    <pin direction="pwr" name="VCCQ6"/>
                    <pin direction="pwr" name="VCCQ7"/>
                    <pin direction="pwr" name="VCCQ8"/>
                    <pin direction="io" name="DQ0-2"/>
                    <pin direction="io" name="DQ0-1"/>
                    <pin direction="io" name="DQ1-2"/>
                    <pin direction="io" name="DQ1-1"/>
                    <pin direction="io" name="DQ2-2"/>
                    <pin direction="io" name="DQ2-1"/>
                    <pin direction="io" name="DQ3-2"/>
                    <pin direction="io" name="DQ3-1"/>
                    <pin direction="io" name="DQ4-2"/>
                    <pin direction="io" name="DQ4-1"/>
                    <pin direction="io" name="DQ5-2"/>
                    <pin direction="io" name="DQ5-1"/>
                    <pin direction="io" name="DQ6-2"/>
                    <pin direction="io" name="DQ6-1"/>
                    <pin direction="io" name="DQ7-2"/>
                    <pin direction="io" name="DQ7-1"/>
                    <pin direction="in" name="!CE"/>
                    <pin direction="in" name="!CE2"/>
                    <pin direction="in" name="!CE3"/>
                    <pin direction="in" name="!CE4"/>
                    <pin direction="in" name="!RE-2(W/!R-2)"/>
                    <pin direction="in" name="!RE-1(W/!R-1)"/>
                    <pin direction="in" name="!WE-2(CLK-2)"/>
                    <pin direction="in" name="!WE-1(CLK-1)"/>
                    <pin direction="in" name="!WP-2"/>
                    <pin direction="in" name="!WP-1"/>
                    <pin direction="io" name="N/A(DQS-2)"/>
                    <pin direction="io" name="N/A(DQS-1)"/>
                    <pin direction="oc" name="R/!B"/>
                    <pin name="R/!B2"/>
                    <pin direction="oc" name="R/!B3"/>
                    <pin name="R/!B4"/>
                    <pin direction="in" name="ALE-2"/>
                    <pin direction="in" name="ALE-1"/>
                    <pin direction="in" name="CLE-2"/>
                    <pin direction="in" name="CLE-1"/>
                    <pin direction="pas" name="NC10"/>
                    <pin direction="pas" name="NC"/>
                    <pin direction="pas" name="NC3"/>
                    <pin direction="pas" name="NC4"/>
                    <pin direction="pas" name="NC5"/>
                    <pin direction="pas" name="NC6"/>
                    <pin direction="pas" name="NC7"/>
                    <pin direction="pas" name="NC8"/>
                    <pin direction="pas" name="NC9"/>
                    <pin direction="pas" name="NC2"/>
                    <pin direction="pas" name="NC11"/>
                    <pin direction="pas" name="NC12"/>
                    <pin direction="pas" name="NC13"/>
                    <pin direction="pas" name="NC14"/>
                    <pin direction="pas" name="NC15"/>
                    <pin direction="pas" name="NC16"/>
                    <pin direction="pas" name="NC17"/>
                    <pin direction="pas" name="NC18"/>
                </symbol>
            </symbols>
            <devicesets>
                <deviceset prefix="Q" name="ON_SEMI_MMBT4401LT3G">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="ON_SEMI_MMBT4401LT3G_0_0"/>
                    </gates>
                    <devices>
                        <device name="ON_SEMI_MMBT4401LT3G_0_0" package="ON_SEMI_MMBT4401LT3G_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="BASE"/>
                                <connect gate="G$0" pad="2" pin="EMITTER"/>
                                <connect gate="G$0" pad="3" pin="COLLECTOR"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="Current_-_Collector_(Ic)_(Max)" value="600mA"/>
                                    <attribute name="mouser_part_number" value="863-MMBT4401LT3G"/>
                                    <attribute name="ipc_land_pattern_name" value="SOT95P240X100-3"/>
                                    <attribute name="temperature_range_high" value="+150°C"/>
                                    <attribute name="MPN" value="MMBT4401LT3G"/>
                                    <attribute name="digikey_description" value="TRANS Bipolar (BJT) Transistor NPN 40V 600mA 250MHz 300mW Surface Mount SOT-23-3 (TO-236)"/>
                                    <attribute name="digikey_part_number" value="MMBT4401LT3GOSCT-ND"/>
                                    <attribute name="prefix" value="Q"/>
                                    <attribute name="Voltage_-_Collector_Emitter_Breakdown_(Max)" value="40V"/>
                                    <attribute name="datasheet" value="http://www.onsemi.ru.com/pub_link/Collateral/MMBT4401LT1-D.PDF"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="mfg_package_ident" value="CASE 318−08 ISSUE AR"/>
                                    <attribute name="Power_(max)" value="300mW"/>
                                    <attribute name="voltage" value=""/>
                                    <attribute name="temperature_range_low" value="-55°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="MF" value="ON Semi"/>
                                    <attribute name="package" value="SOT−23"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="J" name="HIROSE_DF11CZ-16DS-2V_22">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="HIROSE_DF11CZ-16DS-2V_22_0_0"/>
                    </gates>
                    <devices>
                        <device name="HIROSE_DF11CZ-16DS-2V_22_0_0" package="HIROSE_DF11CZ-16DS-2V_22_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="1"/>
                                <connect gate="G$0" pad="2" pin="2"/>
                                <connect gate="G$0" pad="3" pin="3"/>
                                <connect gate="G$0" pad="4" pin="4"/>
                                <connect gate="G$0" pad="5" pin="5"/>
                                <connect gate="G$0" pad="6" pin="6"/>
                                <connect gate="G$0" pad="7" pin="7"/>
                                <connect gate="G$0" pad="8" pin="8"/>
                                <connect gate="G$0" pad="9" pin="9"/>
                                <connect gate="G$0" pad="10" pin="10"/>
                                <connect gate="G$0" pad="11" pin="11"/>
                                <connect gate="G$0" pad="12" pin="12"/>
                                <connect gate="G$0" pad="13" pin="13"/>
                                <connect gate="G$0" pad="14" pin="14"/>
                                <connect gate="G$0" pad="15" pin="15"/>
                                <connect gate="G$0" pad="16" pin="16"/>
                                <connect gate="G$0" pad="17" pin="MNT_1"/>
                                <connect gate="G$0" pad="18" pin="MNT_2"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="MPN" value="DF11CZ-16DS-2V(22)"/>
                                    <attribute name="mouser_part_number" value="798-DF11CZ16DS2V22"/>
                                    <attribute name="forked_from" value="63dcb37d11d876c8"/>
                                    <attribute name="digikey_description" value='CONN 16 Position Receptacle Connector 0.079" (2.00mm) Surface Mount Tin'/>
                                    <attribute name="MF" value="HIROSE"/>
                                    <attribute name="digikey_part_number" value="DF11CZ-16DS-2V(22)-ND"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="prefix" value="J"/>
                                    <attribute name="is_female" value="yes"/>
                                    <attribute name="package" value="HDR16"/>
                                    <attribute name="temperature_range_low" value="-40℃"/>
                                    <attribute name="datasheet" value="https://www.hirose.com/product/en/download_file/key_name/DF11CZ-16DS-2V%2822%29/category/Drawing%20(2D)/doc_file_id/39833/?file_category_id=6&amp;item_id=05432069722&amp;is_series="/>
                                    <attribute name="temperature_range_high" value="+85℃"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="U" name="MICROCHIP_93LC56B-I-SN">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="MICROCHIP_93LC56B-I-SN_0_0"/>
                    </gates>
                    <devices>
                        <device name="MICROCHIP_93LC56B-I-SN_0_0" package="MICROCHIP_93LC56B-I-SN_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="CS"/>
                                <connect gate="G$0" pad="2" pin="CLK"/>
                                <connect gate="G$0" pad="3" pin="DI"/>
                                <connect gate="G$0" pad="4" pin="DO"/>
                                <connect gate="G$0" pad="5" pin="VSS"/>
                                <connect gate="G$0" pad="6" pin="NC"/>
                                <connect gate="G$0" pad="7" pin="NC2"/>
                                <connect gate="G$0" pad="8" pin="VCC"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="reach_svhc_compliance" value="No SVHC"/>
                                    <attribute name="mouser_part_number" value="579-93LC56BISN"/>
                                    <attribute name="footprint_2_description" value="SOIC, 8-Leads, Body 4.9x3.8mm, Pitch 1.27mm, IPC Low Density"/>
                                    <attribute name="frequency" value="2000000.0Hz"/>
                                    <attribute name="max_supply_voltage_dc" value="5.5V"/>
                                    <attribute name="operating_voltage" value="2.5V"/>
                                    <attribute name="temperature_range_high" value="+85°C"/>
                                    <attribute name="MPN" value="93LC56B-I/SN"/>
                                    <attribute name="digikey_description" value="IC EEPROM 2KBIT 2MHZ 8SOIC"/>
                                    <attribute name="digikey_part_number" value="93LC56B-I/SN-ND"/>
                                    <attribute name="clock_speed" value="2000000.0Hz"/>
                                    <attribute name="supply_voltage_dc" value="5.0V"/>
                                    <attribute name="prefix" value="U"/>
                                    <attribute name="datasheet" value="http://ww1.microchip.com/downloads/en/DeviceDoc/21794F.pdf"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="Packaging_Specification" value="http://www.microchip.com/stellent/groups/techpub_sg/documents/packagingspec/en012702.pdf"/>
                                    <attribute name="mfg_package_ident" value="C04-2057A"/>
                                    <attribute name="mounting_style" value="surface mount"/>
                                    <attribute name="imported_from" value="Altium"/>
                                    <attribute name="temperature_range_low" value="-40°C"/>
                                    <attribute name="footprint_0_description" value="SOIC, 8-Leads, Body 4.9x3.8mm, Pitch 1.27mm, IPC Medium Density"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="Microchipcom_Home" value="http://www.microchip.com/"/>
                                    <attribute name="ipc_land_pattern_name" value="SOIC127P600X175-8"/>
                                    <attribute name="octopart_part_number" value="ccff05f497701338"/>
                                    <attribute name="MF" value="Microchip"/>
                                    <attribute name="package" value="SOIC8"/>
                                    <attribute name="footprint_1_description" value="SOIC, 8-Leads, Body 4.9x3.8mm, Pitch 1.27mm, IPC High Density"/>
                                    <attribute name="PackageDescription" value="8-Lead Plastic Small Outline (SN) - Narrow, 3.90mm Body [SOIC]"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="J" name="JST_BM12B-SRSS-TB_LF_SN">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="JST_BM12B-SRSS-TB_LF_SN_0_0"/>
                    </gates>
                    <devices>
                        <device name="JST_BM12B-SRSS-TB_LF_SN_0_0" package="JST_BM12B-SRSS-TB_LF_SN_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="1"/>
                                <connect gate="G$0" pad="2" pin="2"/>
                                <connect gate="G$0" pad="3" pin="3"/>
                                <connect gate="G$0" pad="4" pin="4"/>
                                <connect gate="G$0" pad="5" pin="5"/>
                                <connect gate="G$0" pad="6" pin="6"/>
                                <connect gate="G$0" pad="7" pin="7"/>
                                <connect gate="G$0" pad="8" pin="8"/>
                                <connect gate="G$0" pad="9" pin="9"/>
                                <connect gate="G$0" pad="10" pin="10"/>
                                <connect gate="G$0" pad="11" pin="11"/>
                                <connect gate="G$0" pad="12" pin="12"/>
                                <connect gate="G$0" pad="13" pin="MNT_1"/>
                                <connect gate="G$0" pad="14" pin="MNT_2"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="description" value=""/>
                                    <attribute name="temperature_range_high" value="+85↑8C"/>
                                    <attribute name="MPN" value="BM12B-SRSS-TB(LF)(SN)"/>
                                    <attribute name="digikey_description" value='CONN 12 Positions Header, Shrouded Connector 0.039" (1.00mm) Surface Mount Tin'/>
                                    <attribute name="digikey_part_number" value="455-1798-1-ND"/>
                                    <attribute name="prefix" value="J"/>
                                    <attribute name="datasheet" value="http://www.jst-mfg.com/product/pdf/eng/eSH.pdf"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="package" value="HDR12"/>
                                    <attribute name="temperature_range_low" value="-25°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="MF" value="JST"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="U" name="SAMSUNG_SIP-007AFS001">
                    <description></description>
                    <gates>
                        <gate name="C" symbol="SAMSUNG_SIP-007AFS001_0_0"/>
                        <gate name="A" symbol="SAMSUNG_SIP-007AFS001_0_1"/>
                        <gate name="B" symbol="SAMSUNG_SIP-007AFS001_0_2"/>
                        <gate name="D" symbol="SAMSUNG_SIP-007AFS001_0_3"/>
                        <gate name="E" symbol="SAMSUNG_SIP-007AFS001_0_4"/>
                    </gates>
                    <devices>
                        <device name="SAMSUNG_SIP-007AFS001_0_0" package="SAMSUNG_SIP-007AFS001_0">
                            <connects>
                                <connect gate="C" pad="PA1" pin="GMAC_TXEN"/>
                                <connect gate="C" pad="PA2" pin="GMAC_TXD1"/>
                                <connect gate="C" pad="PA3" pin="GMAC_TXD3"/>
                                <connect gate="A" pad="PA4" pin="GND"/>
                                <connect gate="C" pad="PA5" pin="GMAC_GTXCLK"/>
                                <connect gate="C" pad="PA6" pin="GMAC_RXDV"/>
                                <connect gate="C" pad="PA7" pin="GMAC_RXD2"/>
                                <connect gate="C" pad="PA8" pin="GMAC_RXD0"/>
                                <connect gate="A" pad="PA9" pin="GND2"/>
                                <connect gate="B" pad="PA10" pin="AP_MIPICSI_DNCLK"/>
                                <connect gate="B" pad="PA11" pin="AP_MIPICSI_DN0"/>
                                <connect gate="B" pad="PA12" pin="AP_MIPICSI_DN1"/>
                                <connect gate="B" pad="PA13" pin="AP_MIPICSI_DN2"/>
                                <connect gate="B" pad="PA14" pin="AP_MIPICSI_DN3"/>
                                <connect gate="B" pad="PA16" pin="AP_MIPIDSI_DNCLK"/>
                                <connect gate="B" pad="PA17" pin="AP_MIPIDSI_DN0"/>
                                <connect gate="B" pad="PA18" pin="AP_MIPIDSI_DN1"/>
                                <connect gate="B" pad="PA19" pin="AP_MIPIDSI_DN2"/>
                                <connect gate="B" pad="PA20" pin="AP_MIPIDSI_DN3"/>
                                <connect gate="A" pad="PA21" pin="GND3"/>
                                <connect gate="E" pad="PA22" pin="AP_LVDS_TN0"/>
                                <connect gate="E" pad="PA23" pin="AP_LVDS_TN1"/>
                                <connect gate="E" pad="PA24" pin="AP_LVDS_TN2"/>
                                <connect gate="E" pad="PA25" pin="AP_LVDS_TNCLK"/>
                                <connect gate="E" pad="PA26" pin="AP_LVDS_TN3"/>
                                <connect gate="E" pad="PA27" pin="AP_LVDS_TN4"/>
                                <connect gate="A" pad="PA28" pin="GND4"/>
                                <connect gate="D" pad="PA29" pin="AP_HDMI_CEC"/>
                                <connect gate="D" pad="PA30" pin="AP_HDMI_TX2N"/>
                                <connect gate="D" pad="PA31" pin="AP_HDMI_TX1N"/>
                                <connect gate="D" pad="PA32" pin="AP_HDMI_TX0N"/>
                                <connect gate="D" pad="PA33" pin="AP_HDMI_TXCN"/>
                                <connect gate="A" pad="PA34" pin="GND5"/>
                                <connect gate="E" pad="PA35" pin="AP_OTG_DM"/>
                                <connect gate="E" pad="PA36" pin="AP_USBH_DM"/>
                                <connect gate="C" pad="PA37" pin="AP_GPA13"/>
                                <connect gate="D" pad="PA38" pin="AP_HSIC_STROBE"/>
                                <connect gate="C" pad="PA39" pin="AP_GPA14"/>
                                <connect gate="C" pad="PA40" pin="AP_GPA9"/>
                                <connect gate="C" pad="PA41" pin="AP_GPA15"/>
                                <connect gate="C" pad="PA42" pin="AP_GPA12"/>
                                <connect gate="A" pad="PA43" pin="GND6"/>
                                <connect gate="A" pad="PB1" pin="GND7"/>
                                <connect gate="C" pad="PB2" pin="GMAC_TXD0"/>
                                <connect gate="C" pad="PB3" pin="GMAC_TXD2"/>
                                <connect gate="C" pad="PB4" pin="GMAC_MDC"/>
                                <connect gate="C" pad="PB5" pin="GMAC_RXCLK"/>
                                <connect gate="C" pad="PB6" pin="GMAC_RXD3"/>
                                <connect gate="C" pad="PB7" pin="GMAC_RXD1"/>
                                <connect gate="C" pad="PB8" pin="GMAC_MDIO"/>
                                <connect gate="A" pad="PB9" pin="GND8"/>
                                <connect gate="B" pad="PB10" pin="AP_MIPICSI_DPCLK"/>
                                <connect gate="B" pad="PB11" pin="AP_MIPICSI_DP0"/>
                                <connect gate="B" pad="PB12" pin="AP_MIPICSI_DP1"/>
                                <connect gate="B" pad="PB13" pin="AP_MIPICSI_DP2"/>
                                <connect gate="B" pad="PB14" pin="AP_MIPICSI_DP3"/>
                                <connect gate="A" pad="PB15" pin="GND9"/>
                                <connect gate="B" pad="PB16" pin="AP_MIPIDSI_DPCLK"/>
                                <connect gate="B" pad="PB17" pin="AP_MIPIDSI_DP0"/>
                                <connect gate="B" pad="PB18" pin="AP_MIPIDSI_DP1"/>
                                <connect gate="B" pad="PB19" pin="AP_MIPIDSI_DP2"/>
                                <connect gate="B" pad="PB20" pin="AP_MIPIDSI_DP3"/>
                                <connect gate="A" pad="PB21" pin="GND10"/>
                                <connect gate="E" pad="PB22" pin="AP_LVDS_TP0"/>
                                <connect gate="E" pad="PB23" pin="AP_LVDS_TP1"/>
                                <connect gate="E" pad="PB24" pin="AP_LVDS_TP2"/>
                                <connect gate="E" pad="PB25" pin="AP_LVDS_TPCLK"/>
                                <connect gate="E" pad="PB26" pin="AP_LVDS_TP3"/>
                                <connect gate="E" pad="PB27" pin="AP_LVDS_TP4"/>
                                <connect gate="A" pad="PB28" pin="GND11"/>
                                <connect gate="D" pad="PB29" pin="AP_HDMI_HPD"/>
                                <connect gate="D" pad="PB30" pin="AP_HDMI_TX2P"/>
                                <connect gate="D" pad="PB31" pin="AP_HDMI_TX1P"/>
                                <connect gate="D" pad="PB32" pin="AP_HDMI_TX0P"/>
                                <connect gate="D" pad="PB33" pin="AP_HDMI_TXCP"/>
                                <connect gate="A" pad="PB34" pin="GND12"/>
                                <connect gate="E" pad="PB35" pin="AP_OTG_DP"/>
                                <connect gate="E" pad="PB36" pin="AP_USBH_DP"/>
                                <connect gate="E" pad="PB37" pin="AP_OTG_ID"/>
                                <connect gate="D" pad="PB38" pin="AP_HSIC_DATA"/>
                                <connect gate="C" pad="PB39" pin="AP_GPA4"/>
                                <connect gate="C" pad="PB40" pin="AP_GPA5"/>
                                <connect gate="C" pad="PB41" pin="AP_GPA16"/>
                                <connect gate="C" pad="PB42" pin="AP_GPA11"/>
                                <connect gate="A" pad="PB43" pin="GND13"/>
                                <connect gate="A" pad="PC1" pin="GND14"/>
                                <connect gate="A" pad="PC42" pin="GND15"/>
                                <connect gate="A" pad="PC43" pin="GND16"/>
                                <connect gate="A" pad="PD1" pin="GND17"/>
                                <connect gate="A" pad="PD42" pin="VCC5P0_OTGVBUS"/>
                                <connect gate="A" pad="PD43" pin="VCC5P0_OTGVBUS2"/>
                                <connect gate="A" pad="PE1" pin="GND18"/>
                                <connect gate="A" pad="PE2" pin="GND19"/>
                                <connect gate="A" pad="PE42" pin="VCC2P8_LDO7"/>
                                <connect gate="A" pad="PE43" pin="VCC2P8_LDO72"/>
                                <connect gate="A" pad="PF1" pin="GND20"/>
                                <connect gate="A" pad="PF2" pin="GND21"/>
                                <connect gate="A" pad="PF42" pin="VCC2P8_LDO73"/>
                                <connect gate="A" pad="PF43" pin="GND22"/>
                                <connect gate="A" pad="PG1" pin="GND23"/>
                                <connect gate="A" pad="PG42" pin="GND24"/>
                                <connect gate="A" pad="PG43" pin="GND25"/>
                                <connect gate="A" pad="PH1" pin="GND26"/>
                                <connect gate="A" pad="PH42" pin="VCC_LDO5"/>
                                <connect gate="A" pad="PH43" pin="VCC_LDO52"/>
                                <connect gate="A" pad="PJ1" pin="GND27"/>
                                <connect gate="A" pad="PJ2" pin="GND28"/>
                                <connect gate="A" pad="PJ42" pin="VCC_LDO53"/>
                                <connect gate="A" pad="PJ43" pin="VCC_LDO2"/>
                                <connect gate="A" pad="PK1" pin="GND29"/>
                                <connect gate="A" pad="PK2" pin="GND30"/>
                                <connect gate="A" pad="PK42" pin="VCC_LDO22"/>
                                <connect gate="A" pad="PK43" pin="VCC_LDO23"/>
                                <connect gate="A" pad="PL1" pin="GND31"/>
                                <connect gate="A" pad="PL2" pin="GND32"/>
                                <connect gate="A" pad="PL42" pin="GND33"/>
                                <connect gate="A" pad="PL43" pin="GND34"/>
                                <connect gate="A" pad="PM1" pin="GND35"/>
                                <connect gate="A" pad="PM2" pin="GND36"/>
                                <connect gate="A" pad="PM42" pin="VCC_LDO1"/>
                                <connect gate="A" pad="PM43" pin="VCC_LDO12"/>
                                <connect gate="A" pad="PN1" pin="GND37"/>
                                <connect gate="A" pad="PN2" pin="GND38"/>
                                <connect gate="A" pad="PN42" pin="VCC_LDO13"/>
                                <connect gate="A" pad="PN43" pin="GND39"/>
                                <connect gate="A" pad="PP1" pin="GND40"/>
                                <connect gate="A" pad="PP42" pin="VCC1P2_LDO10"/>
                                <connect gate="A" pad="PP43" pin="GND41"/>
                                <connect gate="A" pad="PR1" pin="GND42"/>
                                <connect gate="A" pad="PR2" pin="GND43"/>
                                <connect gate="A" pad="PR42" pin="VCC1P2_LDO102"/>
                                <connect gate="A" pad="PR43" pin="VCC1P2_LDO103"/>
                                <connect gate="A" pad="PT1" pin="VCC1P8_LDO4"/>
                                <connect gate="A" pad="PT2" pin="GND44"/>
                                <connect gate="A" pad="PT42" pin="VCC_LDO9"/>
                                <connect gate="A" pad="PT43" pin="GND45"/>
                                <connect gate="A" pad="PU1" pin="VCC1P8_LDO42"/>
                                <connect gate="A" pad="PU42" pin="VCC_LDO92"/>
                                <connect gate="A" pad="PU43" pin="VCC_LDO93"/>
                                <connect gate="A" pad="PV1" pin="VCC1P8_LDO43"/>
                                <connect gate="A" pad="PV42" pin="VBAT_MAIN"/>
                                <connect gate="A" pad="PV43" pin="VBAT_MAIN2"/>
                                <connect gate="B" pad="PW1" pin="AP_ADC4"/>
                                <connect gate="B" pad="PW2" pin="AP_ADC5"/>
                                <connect gate="A" pad="PW42" pin="VBAT_MAIN3"/>
                                <connect gate="A" pad="PW43" pin="VBAT_MAIN4"/>
                                <connect gate="B" pad="PY1" pin="AP_ADC0"/>
                                <connect gate="B" pad="PY2" pin="AP_ADC1"/>
                                <connect gate="A" pad="PY42" pin="VBAT_MAIN5"/>
                                <connect gate="A" pad="PY43" pin="VBAT_MAIN6"/>
                                <connect gate="B" pad="PAA1" pin="AP_ADC2"/>
                                <connect gate="B" pad="PAA2" pin="AP_ADC3"/>
                                <connect gate="A" pad="PAA42" pin="VBAT_MAIN7"/>
                                <connect gate="A" pad="PAA43" pin="VBAT_MAIN8"/>
                                <connect gate="A" pad="PAB1" pin="GND46"/>
                                <connect gate="A" pad="PAB2" pin="GND47"/>
                                <connect gate="A" pad="PAB42" pin="VBAT_MAIN9"/>
                                <connect gate="A" pad="PAB43" pin="VBAT_MAIN10"/>
                                <connect gate="D" pad="PAC1" pin="AP_TCK"/>
                                <connect gate="D" pad="PAC2" pin="AP_TMS"/>
                                <connect gate="A" pad="PAC42" pin="GND48"/>
                                <connect gate="A" pad="PAC43" pin="GND49"/>
                                <connect gate="D" pad="PAD1" pin="AP_TDO"/>
                                <connect gate="D" pad="PAD2" pin="AP_TDI"/>
                                <connect gate="A" pad="PAD42" pin="VCC3V3_LDO8"/>
                                <connect gate="A" pad="PAD43" pin="VCC3V3_LDO82"/>
                                <connect gate="D" pad="PAE1" pin="AP_NTRST"/>
                                <connect gate="D" pad="PAE2" pin="AP_AGP2_RTC_INT_N"/>
                                <connect gate="A" pad="PAE42" pin="GND50"/>
                                <connect gate="A" pad="PAE43" pin="VCC3V3_LDO83"/>
                                <connect gate="D" pad="PAF1" pin="AP_PWRKEY"/>
                                <connect gate="D" pad="PAF2" pin="AP_AGP1_HOMEKEY"/>
                                <connect gate="A" pad="PAF42" pin="GND51"/>
                                <connect gate="A" pad="PAF43" pin="GND52"/>
                                <connect gate="D" pad="PAG1" pin="AP_NRESET"/>
                                <connect gate="D" pad="PAG2" pin="AP_GPA25_BACKKEY"/>
                                <connect gate="C" pad="PAG42" pin="AP_GPB11"/>
                                <connect gate="C" pad="PAG43" pin="AP_GPB18"/>
                                <connect gate="D" pad="PAH1" pin="AP_GPA26_VOLUP"/>
                                <connect gate="D" pad="PAH2" pin="AP_GPA0_MENUKEY"/>
                                <connect gate="C" pad="PAH42" pin="AP_GPC25"/>
                                <connect gate="C" pad="PAH43" pin="AP_GPE31"/>
                                <connect gate="D" pad="PAJ1" pin="AP_I2S0_LRCLK"/>
                                <connect gate="D" pad="PAJ2" pin="AP_GPA27_VOLDOWN"/>
                                <connect gate="B" pad="PAJ42" pin="BT_PCM_D_OUT"/>
                                <connect gate="B" pad="PAJ43" pin="BT_PCM_LRCK"/>
                                <connect gate="D" pad="PAK1" pin="AP_I2S0_DOUT"/>
                                <connect gate="D" pad="PAK2" pin="AP_I2S0_BCLK"/>
                                <connect gate="E" pad="PAK3" pin="AP_GPC11_SPI2_MISO"/>
                                <connect gate="E" pad="PAK4" pin="AP_GPC9_SPI2_CLK"/>
                                <connect gate="E" pad="PAK5" pin="AP_SPI0_MISO"/>
                                <connect gate="E" pad="PAK6" pin="AP_SPI0_CLK"/>
                                <connect gate="E" pad="PAK7" pin="AP_GPC14_PWM2"/>
                                <connect gate="D" pad="PAK8" pin="AP_GPD6_SCL"/>
                                <connect gate="D" pad="PAK9" pin="AP_GPD4_SCL1"/>
                                <connect gate="D" pad="PAK10" pin="AP_GPD2_SCL0"/>
                                <connect gate="D" pad="PAK11" pin="AP_GPA23_HDMI_I2C_SCL"/>
                                <connect gate="E" pad="PAK12" pin="ZB_JTMS"/>
                                <connect gate="E" pad="PAK13" pin="ZB_JTCK"/>
                                <connect gate="E" pad="PAK14" pin="ZB_PC0"/>
                                <connect gate="E" pad="PAK15" pin="ZB_PA4"/>
                                <connect gate="A" pad="PAK16" pin="GND53"/>
                                <connect gate="A" pad="PAK17" pin="VCC3P3_SYS"/>
                                <connect gate="A" pad="PAK18" pin="VCC3P3_SYS2"/>
                                <connect gate="E" pad="PAK19" pin="AP_NBATTF"/>
                                <connect gate="E" pad="PAK20" pin="AP_GPE2"/>
                                <connect gate="E" pad="PAK21" pin="AP_GPE1"/>
                                <connect gate="E" pad="PAK22" pin="AP_UARTTX3"/>
                                <connect gate="E" pad="PAK23" pin="AP_UARTTX4"/>
                                <connect gate="E" pad="PAK24" pin="AP_UARTTX5"/>
                                <connect gate="D" pad="PAK25" pin="AP_GPB0_VID1_1_I2SLRCK1"/>
                                <connect gate="D" pad="PAK26" pin="AP_GPA28_I2SMCLK1"/>
                                <connect gate="D" pad="PAK27" pin="AP_GPA30_VID1_0_I2SBCLK1"/>
                                <connect gate="E" pad="PAK28" pin="AP_SD0_CMD"/>
                                <connect gate="E" pad="PAK29" pin="AP_SD0_D1"/>
                                <connect gate="E" pad="PAK30" pin="AP_SD0_CLK"/>
                                <connect gate="B" pad="PAK31" pin="AP_DISD6_BOOT"/>
                                <connect gate="B" pad="PAK32" pin="AP_GPB13_SD0_BOOT"/>
                                <connect gate="C" pad="PAK33" pin="AP_GPC17"/>
                                <connect gate="C" pad="PAK34" pin="AP_GPC0"/>
                                <connect gate="C" pad="PAK35" pin="AP_GPC26"/>
                                <connect gate="C" pad="PAK36" pin="AP_GPB8"/>
                                <connect gate="E" pad="PAK37" pin="AP_GPB14"/>
                                <connect gate="C" pad="PAK38" pin="AP_GPA20"/>
                                <connect gate="C" pad="PAK39" pin="AP_GPA18"/>
                                <connect gate="C" pad="PAK40" pin="AP_GPA21"/>
                                <connect gate="C" pad="PAK41" pin="AP_GPA10"/>
                                <connect gate="C" pad="PAK42" pin="AP_GPA6"/>
                                <connect gate="B" pad="PAK43" pin="BT_PCM_D_IN"/>
                                <connect gate="D" pad="PAL1" pin="AP_I2S0_DIN"/>
                                <connect gate="D" pad="PAL2" pin="AP_I2S0_MCLK"/>
                                <connect gate="E" pad="PAL3" pin="AP_GPC12_SPI2_MOSI"/>
                                <connect gate="E" pad="PAL4" pin="AP_GPC10_SPI2_CS"/>
                                <connect gate="E" pad="PAL5" pin="AP_SPI0_MOSI"/>
                                <connect gate="E" pad="PAL6" pin="AP_SPI0_CS"/>
                                <connect gate="E" pad="PAL7" pin="AP_GPD1_PWM0"/>
                                <connect gate="D" pad="PAL8" pin="AP_GPD7_SDA"/>
                                <connect gate="D" pad="PAL9" pin="AP_GPD5_SDA1"/>
                                <connect gate="D" pad="PAL10" pin="AP_GPD3_SDA0"/>
                                <connect gate="D" pad="PAL11" pin="AP_GPA24_HDMI_I2C_SDA"/>
                                <connect gate="E" pad="PAL12" pin="ZB_JTDI"/>
                                <connect gate="E" pad="PAL13" pin="ZB_JTDO"/>
                                <connect gate="E" pad="PAL14" pin="ZB_RSTN"/>
                                <connect gate="E" pad="PAL15" pin="ZB_PA5"/>
                                <connect gate="A" pad="PAL16" pin="GND54"/>
                                <connect gate="A" pad="PAL17" pin="VCC3P3_SYS3"/>
                                <connect gate="A" pad="PAL18" pin="VCC3P3_SYS4"/>
                                <connect gate="E" pad="PAL19" pin="AP_VDDPWRON"/>
                                <connect gate="E" pad="PAL20" pin="AP_GPE3"/>
                                <connect gate="E" pad="PAL21" pin="AP_GPE0"/>
                                <connect gate="E" pad="PAL22" pin="AP_UARTRX3"/>
                                <connect gate="E" pad="PAL23" pin="AP_UARTRX4"/>
                                <connect gate="E" pad="PAL24" pin="AP_UARTRX5"/>
                                <connect gate="E" pad="PAL25" pin="AP_GPD31"/>
                                <connect gate="D" pad="PAL26" pin="AP_GPB9_I2SDIN1"/>
                                <connect gate="D" pad="PAL27" pin="AP_GPB6_VID1_4_I2SDOUT1"/>
                                <connect gate="E" pad="PAL28" pin="AP_SD0_D3"/>
                                <connect gate="E" pad="PAL29" pin="AP_SD0_D2"/>
                                <connect gate="E" pad="PAL30" pin="AP_SD0_D0"/>
                                <connect gate="B" pad="PAL31" pin="AP_GPB4_VID1_3_BOOT"/>
                                <connect gate="B" pad="PAL32" pin="AP_GPB15_SD1_BOOT"/>
                                <connect gate="C" pad="PAL33" pin="AP_GPD8"/>
                                <connect gate="C" pad="PAL34" pin="AP_GPE30"/>
                                <connect gate="C" pad="PAL35" pin="AP_GPC27"/>
                                <connect gate="C" pad="PAL36" pin="AP_GPB22"/>
                                <connect gate="E" pad="PAL37" pin="AP_GPB16"/>
                                <connect gate="C" pad="PAL38" pin="AP_GPB23"/>
                                <connect gate="C" pad="PAL39" pin="AP_GPA22"/>
                                <connect gate="C" pad="PAL40" pin="AP_GPA19"/>
                                <connect gate="C" pad="PAL41" pin="AP_GPA17"/>
                                <connect gate="C" pad="PAL42" pin="AP_GPA3"/>
                                <connect gate="B" pad="PAL43" pin="BT_PCM_CLK"/>
                                <connect gate="A" pad="TP282" pin="TP"/>
                                <connect gate="A" pad="TP283" pin="TP2"/>
                                <connect gate="A" pad="TP284" pin="TP3"/>
                                <connect gate="A" pad="TP285" pin="TP4"/>
                                <connect gate="A" pad="TP286" pin="TP5"/>
                                <connect gate="A" pad="TP287" pin="TP6"/>
                                <connect gate="A" pad="TP288" pin="TP7"/>
                                <connect gate="A" pad="TP289" pin="TP8"/>
                                <connect gate="A" pad="TP290" pin="TP9"/>
                                <connect gate="A" pad="TP291" pin="TP10"/>
                                <connect gate="A" pad="TP292" pin="TP11"/>
                                <connect gate="A" pad="TP293" pin="TP12"/>
                                <connect gate="A" pad="TP294" pin="TP13"/>
                                <connect gate="A" pad="TP295" pin="TP14"/>
                                <connect gate="A" pad="TP296" pin="TP15"/>
                                <connect gate="A" pad="TP297" pin="TP16"/>
                                <connect gate="A" pad="TP298" pin="TP17"/>
                                <connect gate="A" pad="TP299" pin="TP18"/>
                                <connect gate="A" pad="TP300" pin="TP19"/>
                                <connect gate="A" pad="TP301" pin="TP20"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="ipc_land_pattern_name" value="BGA1333N112P43X31_4900X3600X345"/>
                                    <attribute name="temperature_range_high" value="+70 °C"/>
                                    <attribute name="MPN" value="SIP-007AFS001"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="temperature_range_low" value="0°C"/>
                                    <attribute name="digikey_part_number" value="1683-1001-ND"/>
                                    <attribute name="prefix" value="U"/>
                                    <attribute name="datasheet" value="http://media.digikey.com/pdf/Data%20Sheets/Samsung%20PDFs/Artik710_DS.pdf"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="digikey_description" value="IC ARTIK 710 ARTIK MPU ARM® Cortex®-A53 Embedded Evaluation Board"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="MF" value="Samsung"/>
                                    <attribute name="package" value="BGA293"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="R" name="VISHAY_CRCW0805200RFKEA">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="VISHAY_CRCW0805200RFKEA_0_0"/>
                    </gates>
                    <devices>
                        <device name="VISHAY_CRCW0805200RFKEA_0_0" package="VISHAY_CRCW0805200RFKEA_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="1"/>
                                <connect gate="G$0" pad="2" pin="2"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="71-CRCW0805-200-E3"/>
                                    <attribute name="power_rating" value="125 mW"/>
                                    <attribute name="voltage_rating_dc" value="150 V"/>
                                    <attribute name="size_length" value="2 mm"/>
                                    <attribute name="temperature_range_high" value="155°C"/>
                                    <attribute name="MPN" value="CRCW0805200RFKEA"/>
                                    <attribute name="digikey_description" value="RES SMD 200 OHM 1% 1/8W 0805"/>
                                    <attribute name="digikey_part_number" value="541-200CCT-ND"/>
                                    <attribute name="prefix" value="R"/>
                                    <attribute name="resistance" value="200Ω"/>
                                    <attribute name="datasheet" value="http://www.vishay.com/docs/20035/dcrcwe3.pdf"/>
                                    <attribute name="case_package_si" value="2012"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="temperature_coefficient" value="100 ppm/°C"/>
                                    <attribute name="voltage" value="150 V"/>
                                    <attribute name="imported_from" value="octopart"/>
                                    <attribute name="temperature_range_low" value="-55°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="mounting_type" value="surface mount"/>
                                    <attribute name="size_width" value="1.25 mm"/>
                                    <attribute name="power" value="125mW"/>
                                    <attribute name="resistance_tolerance" value="±1%"/>
                                    <attribute name="octopart_part_number" value="51f098f826e68e37"/>
                                    <attribute name="num_pins" value="2"/>
                                    <attribute name="MF" value="Vishay"/>
                                    <attribute name="package" value="0805 (2012 metric)"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="L" name="BOURNS_SRN6045-6R8Y">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="BOURNS_SRN6045-6R8Y_0_0"/>
                    </gates>
                    <devices>
                        <device name="BOURNS_SRN6045-6R8Y_0_0" package="BOURNS_SRN6045-6R8Y_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="1"/>
                                <connect gate="G$0" pad="2" pin="2"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="652-SRN6045-6R8Y"/>
                                    <attribute name="Current_Rating" value="2.8A"/>
                                    <attribute name="Current_-_Saturation" value="3.8A"/>
                                    <attribute name="Tolerance" value="±30%"/>
                                    <attribute name="temperature_range_high" value="+125°C"/>
                                    <attribute name="MPN" value="SRN6045-6R8Y"/>
                                    <attribute name="digikey_description" value="IND FIXED IND 6.8UH 2.8A 47.3 MOHM"/>
                                    <attribute name="digikey_part_number" value="SRN6045-6R8YCT-ND"/>
                                    <attribute name="prefix" value="L"/>
                                    <attribute name="datasheet" value="http://www.bourns.com/docs/Product-Datasheets/SRN6045.pdf"/>
                                    <attribute name="inductance" value="6.8µH"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="imported_from" value="octopart"/>
                                    <attribute name="temperature_range_low" value="-40°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="DC_Resistance_(DCR)" value="47.3 mOhm Max"/>
                                    <attribute name="octopart_part_number" value=""/>
                                    <attribute name="num_pins" value=""/>
                                    <attribute name="MF" value="Bourns"/>
                                    <attribute name="package" value="SMT_INDUCTOR_6MM0_6MM0"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="SW" name="CTS_218-6LPST">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="CTS_218-6LPST_0_0"/>
                    </gates>
                    <devices>
                        <device name="CTS_218-6LPST_0_0" package="CTS_218-6LPST_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="1"/>
                                <connect gate="G$0" pad="2" pin="2"/>
                                <connect gate="G$0" pad="3" pin="3"/>
                                <connect gate="G$0" pad="4" pin="4"/>
                                <connect gate="G$0" pad="5" pin="5"/>
                                <connect gate="G$0" pad="6" pin="6"/>
                                <connect gate="G$0" pad="7" pin="6_ON"/>
                                <connect gate="G$0" pad="8" pin="5_ON"/>
                                <connect gate="G$0" pad="9" pin="4_ON"/>
                                <connect gate="G$0" pad="10" pin="3_ON"/>
                                <connect gate="G$0" pad="11" pin="2_ON"/>
                                <connect gate="G$0" pad="12" pin="1_ON"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="MPN" value="218-6LPST"/>
                                    <attribute name="mouser_part_number" value="774-2186LPST"/>
                                    <attribute name="Current_Rating" value="25mA"/>
                                    <attribute name="package" value="SWITCH_SMT_8MM79X5MM8"/>
                                    <attribute name="digikey_description" value="SWITCH Dip Switch SPST 6 Position Surface Mount Slide (Standard) Actuator 25mA 24VDC"/>
                                    <attribute name="centroid_not_specified" value=""/>
                                    <attribute name="digikey_part_number" value="CT2186LPST-ND"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="prefix" value="SW"/>
                                    <attribute name="MF" value="CTS"/>
                                    <attribute name="voltage" value="24V"/>
                                    <attribute name="temperature_range_low" value="-55°C"/>
                                    <attribute name="datasheet" value="https://upverter.com/datasheet/736375c498935064eddcbcf4a1d54b4fbf9a684d.pdf"/>
                                    <attribute name="temperature_range_high" value="+85°C"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="U" name="TEXAS_INSTRUMENTS_SN74AVC2T244DQMR">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="TEXAS_INSTRUMENTS_SN74AVC2T244DQMR_0_0"/>
                    </gates>
                    <devices>
                        <device name="TEXAS_INSTRUMENTS_SN74AVC2T244DQMR_0_0" package="TEXAS_INSTRUMENTS_SN74AVC2T244DQMR_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="VCCA"/>
                                <connect gate="G$0" pad="2" pin="A1"/>
                                <connect gate="G$0" pad="3" pin="A2"/>
                                <connect gate="G$0" pad="4" pin="!OE"/>
                                <connect gate="G$0" pad="5" pin="GND"/>
                                <connect gate="G$0" pad="6" pin="B2"/>
                                <connect gate="G$0" pad="7" pin="B1"/>
                                <connect gate="G$0" pad="8" pin="VCCB"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="MPN" value="SN74AVC2T244DQMR"/>
                                    <attribute name="mouser_part_number" value="595-SN74AVC2T244DQMR"/>
                                    <attribute name="package" value="X2SON8"/>
                                    <attribute name="digikey_description" value="IC BUS TXRX 2BIT DUAL 8X2SON"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="digikey_part_number" value="296-29674-1-ND"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="prefix" value="U"/>
                                    <attribute name="mfg_package_ident" value="DQM (R-PX2SON-N8)"/>
                                    <attribute name="MF" value="Texas Instruments"/>
                                    <attribute name="voltage" value=""/>
                                    <attribute name="temperature_range_low" value="-40°C"/>
                                    <attribute name="datasheet" value="http://www.ti.com/lit/ds/symlink/sn74avc2t244.pdf"/>
                                    <attribute name="temperature_range_high" value="+85°C"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="Y" name="EPSON_FA-20H_16.0000MF12V-AJ3">
                    <description>MHz Range Crystal Unit</description>
                    <gates>
                        <gate name="G$0" symbol="EPSON_FA-20H_16.0000MF12V-AJ3_0_0"/>
                    </gates>
                    <devices>
                        <device name="EPSON_FA-20H_16.0000MF12V-AJ3_0_0" package="EPSON_FA-20H_16.0000MF12V-AJ3_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="1"/>
                                <connect gate="G$0" pad="2" pin="GND"/>
                                <connect gate="G$0" pad="3" pin="3"/>
                                <connect gate="G$0" pad="4" pin="GND2"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="732-FA-20H16F12V-AJ3"/>
                                    <attribute name="num_pins" value="4"/>
                                    <attribute name="description" value="MHz Range Crystal Unit"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="temperature_range_high" value="+70°C"/>
                                    <attribute name="MPN" value="FA-20H 16.0000MF12V-AJ3"/>
                                    <attribute name="digikey_description" value="CRYSTAL 16.00 MHZ 8.0PF SMD"/>
                                    <attribute name="digikey_part_number" value="FA-20H 16.0000MF12V-AJ3-ND"/>
                                    <attribute name="prefix" value="Y"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="package" value="DFN4"/>
                                    <attribute name="temperature_range_low" value="-20°C"/>
                                    <attribute name="capacitance" value="8.0pF"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="datasheet" value="https://support.epson.biz/td/api/doc_check.php?dl=brief_FA-20H_en.pdf"/>
                                    <attribute name="Frequency" value="16 MHz"/>
                                    <attribute name="MF" value="Epson"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="U" name="SILICON_LABORATORIES_CP2102-GMR">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="SILICON_LABORATORIES_CP2102-GMR_0_0"/>
                    </gates>
                    <devices>
                        <device name="SILICON_LABORATORIES_CP2102-GMR_0_0" package="SILICON_LABORATORIES_CP2102-GMR_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="DCD"/>
                                <connect gate="G$0" pad="2" pin="RI"/>
                                <connect gate="G$0" pad="3" pin="GND"/>
                                <connect gate="G$0" pad="4" pin="D+"/>
                                <connect gate="G$0" pad="5" pin="D-"/>
                                <connect gate="G$0" pad="6" pin="VDD"/>
                                <connect gate="G$0" pad="7" pin="REGIN"/>
                                <connect gate="G$0" pad="8" pin="VBUS"/>
                                <connect gate="G$0" pad="9" pin="!RST"/>
                                <connect gate="G$0" pad="10" pin="NC"/>
                                <connect gate="G$0" pad="11" pin="!SUSPEND"/>
                                <connect gate="G$0" pad="12" pin="SUSPEND"/>
                                <connect gate="G$0" pad="13" pin="NC2"/>
                                <connect gate="G$0" pad="14" pin="NC3"/>
                                <connect gate="G$0" pad="15" pin="NC4"/>
                                <connect gate="G$0" pad="16" pin="NC5"/>
                                <connect gate="G$0" pad="17" pin="NC6"/>
                                <connect gate="G$0" pad="18" pin="NC7"/>
                                <connect gate="G$0" pad="19" pin="NC8"/>
                                <connect gate="G$0" pad="20" pin="NC9"/>
                                <connect gate="G$0" pad="21" pin="NC10"/>
                                <connect gate="G$0" pad="22" pin="NC11"/>
                                <connect gate="G$0" pad="23" pin="CTS"/>
                                <connect gate="G$0" pad="24" pin="RTS"/>
                                <connect gate="G$0" pad="25" pin="RXD"/>
                                <connect gate="G$0" pad="26" pin="TXD"/>
                                <connect gate="G$0" pad="27" pin="DSR"/>
                                <connect gate="G$0" pad="28" pin="DTR"/>
                                <connect gate="G$0" pad="29" pin="GND_PAD"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="634-CP2102-GMR"/>
                                    <attribute name="prefix" value="U"/>
                                    <attribute name="temperature_range_high" value="+85°C"/>
                                    <attribute name="MPN" value="CP2102-GMR"/>
                                    <attribute name="digikey_description" value="IC USB Bridge, USB to UART USB 2.0 UART Interface 28-QFN (5x5)"/>
                                    <attribute name="digikey_part_number" value="336-1160-1-ND"/>
                                    <attribute name="datasheet" value="http://www.silabs.com/Support%20Documents/TechnicalDocs/CP2102-9.pdf"/>
                                    <attribute name="type" value="IC "/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="imported_from" value="Eagle"/>
                                    <attribute name="temperature_range_low" value="-40°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="MF" value="Silicon Laboratories"/>
                                    <attribute name="ipc_land_pattern_name" value="QFN50P500X500X90-28"/>
                                    <attribute name="num_pins" value="29"/>
                                    <attribute name="package" value="QFN-28"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="K" name="IXYS_CPC1927J">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="IXYS_CPC1927J_0_0"/>
                    </gates>
                    <devices>
                        <device name="IXYS_CPC1927J_0_0" package="IXYS_CPC1927J_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="1_DRAIN"/>
                                <connect gate="G$0" pad="2" pin="2_DRAIN"/>
                                <connect gate="G$0" pad="3" pin="CATHODE"/>
                                <connect gate="G$0" pad="4" pin="ANODE"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="849-CPC1927J"/>
                                    <attribute name="Isolation_Voltage" value="2500Vrms"/>
                                    <attribute name="Blocking_Voltage" value="250V"/>
                                    <attribute name="temperature_range_high" value="+85°C"/>
                                    <attribute name="MPN" value="CPC1927J"/>
                                    <attribute name="digikey_description" value="RELAY 250VAC/DC ISOPLUS264"/>
                                    <attribute name="digikey_part_number" value="CPC1927J-ND"/>
                                    <attribute name="prefix" value="K"/>
                                    <attribute name="MF" value="IXYS"/>
                                    <attribute name="datasheet" value="http://www.ixysic.com/home/pdfs.nsf/www/CPC1927.pdf/$file/CPC1927.pdf"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="On-State_Resistance" value="200mΩ"/>
                                    <attribute name="temperature_range_low" value="-40°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="Input_Control_Current" value="100mA"/>
                                    <attribute name="Input_Power_Dissipation" value="150mW"/>
                                    <attribute name="Reverse_Input_Voltage" value="5V"/>
                                    <attribute name="package" value="SIP4"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="U" name="TEXAS_INSTRUMENTS_BQ294700DSGR">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="TEXAS_INSTRUMENTS_BQ294700DSGR_0_0"/>
                    </gates>
                    <devices>
                        <device name="TEXAS_INSTRUMENTS_BQ294700DSGR_0_0" package="TEXAS_INSTRUMENTS_BQ294700DSGR_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="VDD"/>
                                <connect gate="G$0" pad="2" pin="V4"/>
                                <connect gate="G$0" pad="3" pin="V3"/>
                                <connect gate="G$0" pad="4" pin="V2"/>
                                <connect gate="G$0" pad="5" pin="V1"/>
                                <connect gate="G$0" pad="6" pin="VSS"/>
                                <connect gate="G$0" pad="7" pin="CD"/>
                                <connect gate="G$0" pad="8" pin="OUT"/>
                                <connect gate="G$0" pad="9" pin="GND_PAD"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="595-BQ294700DSGR"/>
                                    <attribute name="prefix" value="U"/>
                                    <attribute name="temperature_range_high" value="+85°C"/>
                                    <attribute name="MPN" value="BQ294700DSGR"/>
                                    <attribute name="digikey_description" value="IC Battery Battery Protection IC Lithium-Ion 8-WSON (2x2)"/>
                                    <attribute name="digikey_part_number" value="296-34984-1-ND"/>
                                    <attribute name="datasheet" value="https://upverter.com/datasheet/2987f6110750576c4ea886c5183cd23665a7aad5.pdf"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="mfg_package_ident" value="DSG (S-PWSON-N8)"/>
                                    <attribute name="temperature_range_low" value="-40°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="MF" value="Texas Instruments"/>
                                    <attribute name="package" value="WSON-8"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="U" name="TEXAS_INSTRUMENTS_BQ24259RGER">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="TEXAS_INSTRUMENTS_BQ24259RGER_0_0"/>
                    </gates>
                    <devices>
                        <device name="TEXAS_INSTRUMENTS_BQ24259RGER_0_0" package="TEXAS_INSTRUMENTS_BQ24259RGER_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="VBUS"/>
                                <connect gate="G$0" pad="2" pin="PSEL"/>
                                <connect gate="G$0" pad="3" pin="!PG"/>
                                <connect gate="G$0" pad="4" pin="STAT"/>
                                <connect gate="G$0" pad="5" pin="SCL"/>
                                <connect gate="G$0" pad="6" pin="SDA"/>
                                <connect gate="G$0" pad="7" pin="INT"/>
                                <connect gate="G$0" pad="8" pin="OTG"/>
                                <connect gate="G$0" pad="9" pin="!CE"/>
                                <connect gate="G$0" pad="10" pin="ILIM"/>
                                <connect gate="G$0" pad="11" pin="TS"/>
                                <connect gate="G$0" pad="12" pin="QON"/>
                                <connect gate="G$0" pad="13" pin="BAT"/>
                                <connect gate="G$0" pad="14" pin="BAT2"/>
                                <connect gate="G$0" pad="15" pin="SYS"/>
                                <connect gate="G$0" pad="16" pin="SYS2"/>
                                <connect gate="G$0" pad="17" pin="PGND"/>
                                <connect gate="G$0" pad="18" pin="PGND2"/>
                                <connect gate="G$0" pad="19" pin="SW"/>
                                <connect gate="G$0" pad="20" pin="SW2"/>
                                <connect gate="G$0" pad="21" pin="BTST"/>
                                <connect gate="G$0" pad="22" pin="REGN"/>
                                <connect gate="G$0" pad="23" pin="PMID"/>
                                <connect gate="G$0" pad="24" pin="VBUS2"/>
                                <connect gate="G$0" pad="25" pin="THERMAL_PAD"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="MPN" value="BQ24259RGER"/>
                                    <attribute name="mouser_part_number" value="595-BQ24259RGER"/>
                                    <attribute name="digikey_description" value="IC Charger IC Lithium-Ion/Polymer 24-VQFN (4x4)"/>
                                    <attribute name="MF" value="Texas Instruments"/>
                                    <attribute name="digikey_part_number" value="296-43322-1-ND"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="prefix" value="U"/>
                                    <attribute name="package" value="VQFN24_EP"/>
                                    <attribute name="temperature_range_low" value="-40°C"/>
                                    <attribute name="datasheet" value="http://www.ti.com/lit/ds/symlink/bq24259.pdf"/>
                                    <attribute name="temperature_range_high" value="+85°C"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="ENC" name="BOURNS_PEC16-4220F-S0024">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="BOURNS_PEC16-4220F-S0024_0_0"/>
                    </gates>
                    <devices>
                        <device name="BOURNS_PEC16-4220F-S0024_0_0" package="BOURNS_PEC16-4220F-S0024_0">
                            <connects>
                                <connect gate="G$0" pad="A" pin="A"/>
                                <connect gate="G$0" pad="B" pin="B"/>
                                <connect gate="G$0" pad="C" pin="C"/>
                                <connect gate="G$0" pad="D" pin="D"/>
                                <connect gate="G$0" pad="E" pin="E"/>
                                <connect gate="G$0" pad="1" pin="MNT_1"/>
                                <connect gate="G$0" pad="2" pin="MNT_2"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="652-PEC16-4220FS0024"/>
                                    <attribute name="temperature_range_high" value="+70°C"/>
                                    <attribute name="MPN" value="PEC16-4220F-S0024"/>
                                    <attribute name="octopart_part_number" value="166ddf7c6620c9aa"/>
                                    <attribute name="digikey_description" value="ENCODER ROTARY 24 PULSES/REV PCB"/>
                                    <attribute name="digikey_part_number" value="PEC16-4220F-S0024-ND"/>
                                    <attribute name="prefix" value="ENC"/>
                                    <attribute name="datasheet" value="http://www.bourns.com/data/global/pdfs/pec16.pdf"/>
                                    <attribute name="type" value="integrated circuit"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="mfg_package_ident" value=""/>
                                    <attribute name="imported_from" value="octopart"/>
                                    <attribute name="temperature_range_low" value="-30°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="symbol_0_0" value="Standard"/>
                                    <attribute name="num_pins" value="5"/>
                                    <attribute name="MF" value="Bourns"/>
                                    <attribute name="package" value="PTH_PEC16"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="C" name="AVX_F950J476MPAAQ2">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="AVX_F950J476MPAAQ2_0_0"/>
                    </gates>
                    <devices>
                        <device name="AVX_F950J476MPAAQ2_0_0" package="AVX_F950J476MPAAQ2_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="CATHODE"/>
                                <connect gate="G$0" pad="2" pin="ANODE"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="647-F950J476MPAAQ2"/>
                                    <attribute name="Tolerance" value="±20%"/>
                                    <attribute name="temperature_range_high" value="+125°C"/>
                                    <attribute name="MPN" value="F950J476MPAAQ2"/>
                                    <attribute name="digikey_description" value="CAP 47µF ±20% Conformal Coated Tantalum Capacitors 6.3V 0805 (2012 Metric) 1.1 Ohm"/>
                                    <attribute name="digikey_part_number" value="478-8410-1-ND"/>
                                    <attribute name="prefix" value="C"/>
                                    <attribute name="datasheet" value="https://upverter.com/datasheet/7fa6e435c7aa799d18c934a7f413650da7092219.pdf"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="voltage" value="6.3V"/>
                                    <attribute name="temperature_range_low" value="-55°C"/>
                                    <attribute name="capacitance" value="47µF"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="mounting_type" value="Surface Mount"/>
                                    <attribute name="num_pins" value="2"/>
                                    <attribute name="MF" value="AVX"/>
                                    <attribute name="package" value="0805 (2012 metric)"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="R" name="PANASONIC_ERJ-3EKF22R0V">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="PANASONIC_ERJ-3EKF22R0V_0_0"/>
                    </gates>
                    <devices>
                        <device name="PANASONIC_ERJ-3EKF22R0V_0_0" package="PANASONIC_ERJ-3EKF22R0V_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="1"/>
                                <connect gate="G$0" pad="2" pin="2"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="667-ERJ-3EKF22R0V"/>
                                    <attribute name="Temperature_Coefficient" value="±100ppm/°C"/>
                                    <attribute name="ipc_land_pattern_name" value="RESC16080X45"/>
                                    <attribute name="Tolerance" value="±1%"/>
                                    <attribute name="temperature_range_high" value="+155°C"/>
                                    <attribute name="MPN" value="ERJ-3EKF22R0V"/>
                                    <attribute name="digikey_description" value="RES SMD 22 OHM 1% 1/10W 0603"/>
                                    <attribute name="digikey_part_number" value="P22.0HCT-ND"/>
                                    <attribute name="prefix" value="R"/>
                                    <attribute name="resistance" value="22Ω"/>
                                    <attribute name="datasheet" value="https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C283.pdf"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="mfg_package_ident" value=""/>
                                    <attribute name="voltage" value=""/>
                                    <attribute name="temperature_range_low" value="-55°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="power" value="100mW"/>
                                    <attribute name="MF" value="Panasonic"/>
                                    <attribute name="package" value="0603"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="U" name="ST_MICROELECTRONICS_L7805CDT-TR">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="ST_MICROELECTRONICS_L7805CDT-TR_0_0"/>
                    </gates>
                    <devices>
                        <device name="ST_MICROELECTRONICS_L7805CDT-TR_0_0" package="ST_MICROELECTRONICS_L7805CDT-TR_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="IN"/>
                                <connect gate="G$0" pad="2" pin="GND"/>
                                <connect gate="G$0" pad="3" pin="OUT"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="511-L7805CDT-TR"/>
                                    <attribute name="temperature_range_high" value="+125°C"/>
                                    <attribute name="MPN" value="L7805CDT-TR"/>
                                    <attribute name="digikey_description" value="IC Linear Voltage Regulator IC Positive Fixed 1 Output 5V 1.5A D-Pak"/>
                                    <attribute name="digikey_part_number" value="497-7255-1-ND"/>
                                    <attribute name="prefix" value="U"/>
                                    <attribute name="datasheet" value="http://www.tme.eu/se/Document/f6092a52464df9e2325fb217956cf4b6/L78xx.pdf"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="voltage" value=""/>
                                    <attribute name="temperature_range_low" value="0°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="centroid_not_specified" value=""/>
                                    <attribute name="MF" value="ST Microelectronics"/>
                                    <attribute name="package" value="DPAK"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="U" name="TEXAS_INSTRUMENTS_TLC5955RTQR">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="TEXAS_INSTRUMENTS_TLC5955RTQR_0_0"/>
                    </gates>
                    <devices>
                        <device name="TEXAS_INSTRUMENTS_TLC5955RTQR_0_0" package="TEXAS_INSTRUMENTS_TLC5955RTQR_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="OUTB3"/>
                                <connect gate="G$0" pad="2" pin="OUTR3"/>
                                <connect gate="G$0" pad="3" pin="OUTG3"/>
                                <connect gate="G$0" pad="4" pin="OUTB7"/>
                                <connect gate="G$0" pad="5" pin="OUTR7"/>
                                <connect gate="G$0" pad="6" pin="OUTG7"/>
                                <connect gate="G$0" pad="7" pin="SOUT"/>
                                <connect gate="G$0" pad="8" pin="GND"/>
                                <connect gate="G$0" pad="9" pin="OUTG11"/>
                                <connect gate="G$0" pad="10" pin="OUTR11"/>
                                <connect gate="G$0" pad="11" pin="OUTB11"/>
                                <connect gate="G$0" pad="12" pin="OUTG15"/>
                                <connect gate="G$0" pad="13" pin="OUTR15"/>
                                <connect gate="G$0" pad="14" pin="OUTB15"/>
                                <connect gate="G$0" pad="15" pin="OUTG10"/>
                                <connect gate="G$0" pad="16" pin="OUTR10"/>
                                <connect gate="G$0" pad="17" pin="OUTB10"/>
                                <connect gate="G$0" pad="18" pin="OUTG14"/>
                                <connect gate="G$0" pad="19" pin="OUTR14"/>
                                <connect gate="G$0" pad="20" pin="OUTB14"/>
                                <connect gate="G$0" pad="21" pin="OUTG13"/>
                                <connect gate="G$0" pad="22" pin="OUTR13"/>
                                <connect gate="G$0" pad="23" pin="OUTB13"/>
                                <connect gate="G$0" pad="24" pin="OUTG9"/>
                                <connect gate="G$0" pad="25" pin="OUTR9"/>
                                <connect gate="G$0" pad="26" pin="OUTB9"/>
                                <connect gate="G$0" pad="27" pin="OUTG12"/>
                                <connect gate="G$0" pad="28" pin="OUTR12"/>
                                <connect gate="G$0" pad="29" pin="OUTB12"/>
                                <connect gate="G$0" pad="30" pin="OUTG8"/>
                                <connect gate="G$0" pad="31" pin="OUTR8"/>
                                <connect gate="G$0" pad="32" pin="OUTB8"/>
                                <connect gate="G$0" pad="33" pin="VCC"/>
                                <connect gate="G$0" pad="34" pin="GSCLK"/>
                                <connect gate="G$0" pad="35" pin="GND2"/>
                                <connect gate="G$0" pad="36" pin="SIN"/>
                                <connect gate="G$0" pad="37" pin="SCLK"/>
                                <connect gate="G$0" pad="38" pin="LAT"/>
                                <connect gate="G$0" pad="39" pin="OUTB4"/>
                                <connect gate="G$0" pad="40" pin="OUTR4"/>
                                <connect gate="G$0" pad="41" pin="OUTG4"/>
                                <connect gate="G$0" pad="42" pin="OUTB0"/>
                                <connect gate="G$0" pad="43" pin="OUTR0"/>
                                <connect gate="G$0" pad="44" pin="OUTG0"/>
                                <connect gate="G$0" pad="45" pin="OUTB5"/>
                                <connect gate="G$0" pad="46" pin="OUTR5"/>
                                <connect gate="G$0" pad="47" pin="OUTG5"/>
                                <connect gate="G$0" pad="48" pin="OUTB1"/>
                                <connect gate="G$0" pad="49" pin="OUTR1"/>
                                <connect gate="G$0" pad="50" pin="OUTG1"/>
                                <connect gate="G$0" pad="51" pin="OUTB2"/>
                                <connect gate="G$0" pad="52" pin="OUTR2"/>
                                <connect gate="G$0" pad="53" pin="OUTG2"/>
                                <connect gate="G$0" pad="54" pin="OUTB6"/>
                                <connect gate="G$0" pad="55" pin="OUTR6"/>
                                <connect gate="G$0" pad="56" pin="OUTG6"/>
                                <connect gate="G$0" pad="57" pin="GND_PAD"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="595-TLC5955RTQR"/>
                                    <attribute name="ipc_land_pattern_name" value="QFN50P800X800X90-56"/>
                                    <attribute name="temperature_range_high" value="+85°C"/>
                                    <attribute name="MPN" value="TLC5955RTQR"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="digikey_description" value="IC LED Driver IC 48 Output Linear Shift Register 23.9mA, 31.9mA 56-QFN (8x8)"/>
                                    <attribute name="digikey_part_number" value="296-40588-1-ND"/>
                                    <attribute name="prefix" value="U"/>
                                    <attribute name="Supply_voltage" value="3.0V to 5.5V"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="mfg_package_ident" value="RTQ (S-PVQFN-N56)"/>
                                    <attribute name="temperature_range_low" value="-40°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="datasheet" value="http://www.ti.com/lit/ds/symlink/tlc5955.pdf"/>
                                    <attribute name="mounting_type" value="Surface Mount"/>
                                    <attribute name="Voltage_-_Output" value="10V"/>
                                    <attribute name="MF" value="Texas Instruments"/>
                                    <attribute name="package" value="QFN56"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="D" name="DIODES_MMSZ5233B">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="DIODES_MMSZ5233B_0_0"/>
                    </gates>
                    <devices>
                        <device name="DIODES_MMSZ5233B_0_0" package="DIODES_MMSZ5233B_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="CATHODE"/>
                                <connect gate="G$0" pad="2" pin="ANODE"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="temperature_range_high" value="+150°C"/>
                                    <attribute name="MPN" value="MMSZ5233B"/>
                                    <attribute name="octopart_part_number" value="5d3494a1b61f82f3"/>
                                    <attribute name="digikey_description" value="DIODE ZENER 6V 500MW SOD123"/>
                                    <attribute name="digikey_part_number" value="621-MMSZ5233B-F"/>
                                    <attribute name="prefix" value="D"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="datasheet" value="http://www.diodes.com/_files/datasheets/ds18010.pdf"/>
                                    <attribute name="type" value="diode"/>
                                    <attribute name="mouser_part_number" value="621-MMSZ5233B-F"/>
                                    <attribute name="imported_from" value="octopart"/>
                                    <attribute name="temperature_range_low" value="-65°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="Zener_voltage" value="6V"/>
                                    <attribute name="symbol_0_0" value="Zener Diode"/>
                                    <attribute name="num_pins" value="2"/>
                                    <attribute name="MF" value="Diodes"/>
                                    <attribute name="package" value="SOD123"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="SW" name="E-SWITCH_TL1015AF160QG">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="E-SWITCH_TL1015AF160QG_0_0"/>
                    </gates>
                    <devices>
                        <device name="E-SWITCH_TL1015AF160QG_0_0" package="E-SWITCH_TL1015AF160QG_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="1"/>
                                <connect gate="G$0" pad="2" pin="2"/>
                                <connect gate="G$0" pad="3" pin="G"/>
                                <connect gate="G$0" pad="4" pin="G2"/>
                                <connect gate="G$0" pad="5" pin="G3"/>
                                <connect gate="G$0" pad="6" pin="G4"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="MPN" value="TL1015AF160QG"/>
                                    <attribute name="mouser_part_number" value="612-TL1015AF"/>
                                    <attribute name="package" value="SW_SMT_3MM9_2MM9_TACT"/>
                                    <attribute name="digikey_description" value="SWITCH TACTILE SPST-NO 0.05A 12V"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="digikey_part_number" value="EG4344CT-ND"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="prefix" value="SW"/>
                                    <attribute name="MF" value="E-Switch"/>
                                    <attribute name="voltage" value=""/>
                                    <attribute name="temperature_range_low" value="-20°C"/>
                                    <attribute name="datasheet" value="http://spec_sheets.e-switch.com/specs/P420000.pdf"/>
                                    <attribute name="temperature_range_high" value="+70°C"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="U" name="TEXAS_INSTRUMENTS_AM4376BZDN100">
                    <description></description>
                    <gates>
                        <gate name="A" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_0"/>
                        <gate name="B" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_1"/>
                        <gate name="C" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_2"/>
                        <gate name="D" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_3"/>
                        <gate name="E" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_4"/>
                        <gate name="F" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_5"/>
                        <gate name="G" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_6"/>
                        <gate name="H" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_7"/>
                        <gate name="J" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_8"/>
                        <gate name="K" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_9"/>
                        <gate name="L" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_10"/>
                        <gate name="M" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_11"/>
                        <gate name="N" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_12"/>
                        <gate name="O" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_13"/>
                        <gate name="P" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_14"/>
                        <gate name="Q" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_15"/>
                        <gate name="R" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_16"/>
                        <gate name="S" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_17"/>
                        <gate name="T" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_18"/>
                        <gate name="U" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_19"/>
                        <gate name="V" symbol="TEXAS_INSTRUMENTS_AM4376BZDN100_0_20"/>
                    </gates>
                    <devices>
                        <device name="TEXAS_INSTRUMENTS_AM4376BZDN100_0_0" package="TEXAS_INSTRUMENTS_AM4376BZDN100_0">
                            <connects>
                                <connect gate="B" pad="G24" pin="ECAP0_IN_PWM0_OUT"/>
                                <connect gate="B" pad="G25" pin="EXTINTN"/>
                                <connect gate="B" pad="G22" pin="WARMRSTN"/>
                                <connect gate="B" pad="G20" pin="GPIO5_10"/>
                                <connect gate="B" pad="G21" pin="USB0_DRVVBUS"/>
                                <connect gate="M" pad="G6" pin="VDDS"/>
                                <connect gate="M" pad="G5" pin="VDDS_PLL_DDR"/>
                                <connect gate="O" pad="G4" pin="DDR_D4"/>
                                <connect gate="O" pad="G3" pin="DDR_D5"/>
                                <connect gate="O" pad="G2" pin="DDR_D6"/>
                                <connect gate="O" pad="G1" pin="DDR_D7"/>
                                <connect gate="D" pad="G8" pin="GPMC_A10"/>
                                <connect gate="M" pad="Y19" pin="VDDS2"/>
                                <connect gate="E" pad="Y18" pin="CAM0_DATA2"/>
                                <connect gate="S" pad="Y15" pin="ADC1_AIN5"/>
                                <connect gate="A" pad="Y16" pin="VDDA_ADC1"/>
                                <connect gate="K" pad="Y10" pin="RESERVED"/>
                                <connect gate="S" pad="Y13" pin="ADC0_AIN2"/>
                                <connect gate="S" pad="Y12" pin="ADC0_AIN1"/>
                                <connect gate="R" pad="B25" pin="XTALOUT"/>
                                <connect gate="J" pad="B24" pin="VSS_OSC"/>
                                <connect gate="F" pad="B23" pin="DSS_VSYNC"/>
                                <connect gate="F" pad="B22" pin="DSS_DATA0"/>
                                <connect gate="F" pad="B21" pin="DSS_DATA2"/>
                                <connect gate="F" pad="B20" pin="DSS_DATA5"/>
                                <connect gate="B" pad="J25" pin="UART0_RTSN"/>
                                <connect gate="B" pad="J24" pin="UART0_TXD"/>
                                <connect gate="C" pad="M5" pin="DDR_CSN0"/>
                                <connect gate="C" pad="M4" pin="DDR_CSN1"/>
                                <connect gate="M" pad="M7" pin="VDDS_DDR"/>
                                <connect gate="P" pad="M6" pin="DDR_A10"/>
                                <connect gate="C" pad="M1" pin="DDR_NCK"/>
                                <connect gate="C" pad="M3" pin="DDR_CKE0"/>
                                <connect gate="C" pad="M2" pin="DDR_CK"/>
                                <connect gate="Q" pad="M9" pin="VDD_CORE"/>
                                <connect gate="M" pad="M8" pin="VDDS_DDR2"/>
                                <connect gate="J" pad="P10" pin="VSS"/>
                                <connect gate="J" pad="P11" pin="VSS2"/>
                                <connect gate="J" pad="P12" pin="VSS3"/>
                                <connect gate="J" pad="P13" pin="VSS4"/>
                                <connect gate="J" pad="P14" pin="VSS5"/>
                                <connect gate="J" pad="P15" pin="VSS6"/>
                                <connect gate="Q" pad="P16" pin="VDD_CORE2"/>
                                <connect gate="Q" pad="P17" pin="VDD_CORE3"/>
                                <connect gate="N" pad="P18" pin="VDDSHV3"/>
                                <connect gate="M" pad="P19" pin="VDDS3"/>
                                <connect gate="J" pad="H18" pin="VSS7"/>
                                <connect gate="K" pad="H19" pin="RESERVED2"/>
                                <connect gate="B" pad="M24" pin="MCASP0_AHCLKR"/>
                                <connect gate="B" pad="M25" pin="MCASP0_AXR1"/>
                                <connect gate="M" pad="H12" pin="VDDS4"/>
                                <connect gate="L" pad="H13" pin="VDD_MPU"/>
                                <connect gate="L" pad="H14" pin="VDD_MPU2"/>
                                <connect gate="J" pad="H15" pin="VSS8"/>
                                <connect gate="L" pad="H16" pin="VDD_MPU3"/>
                                <connect gate="N" pad="H17" pin="VDDSHV6"/>
                                <connect gate="T" pad="U24" pin="USB0_ID"/>
                                <connect gate="T" pad="U25" pin="USB1_ID"/>
                                <connect gate="A" pad="U20" pin="VDDA3P3V_USB1"/>
                                <connect gate="A" pad="U21" pin="VDDA1P8V_USB1"/>
                                <connect gate="T" pad="U22" pin="USB1_CE"/>
                                <connect gate="T" pad="U23" pin="USB0_VBUS"/>
                                <connect gate="J" pad="AA23" pin="VSS9"/>
                                <connect gate="G" pad="AA24" pin="TDO"/>
                                <connect gate="G" pad="AA25" pin="TCK"/>
                                <connect gate="T" pad="W24" pin="USB0_DM"/>
                                <connect gate="T" pad="W25" pin="USB0_DP"/>
                                <connect gate="T" pad="W22" pin="USB0_CE"/>
                                <connect gate="J" pad="W23" pin="VSSA_USB"/>
                                <connect gate="A" pad="W20" pin="VDDA3P3V_USB0"/>
                                <connect gate="A" pad="W21" pin="VDDA1P8V_USB0"/>
                                <connect gate="B" pad="E24" pin="GPIO5_13"/>
                                <connect gate="B" pad="E25" pin="GPIO5_12"/>
                                <connect gate="M" pad="E23" pin="VDDS_CLKOUT"/>
                                <connect gate="E" pad="AC20" pin="CAM0_PCLK"/>
                                <connect gate="N" pad="H9" pin="VDDSHV11"/>
                                <connect gate="N" pad="G17" pin="VDDSHV62"/>
                                <connect gate="N" pad="G16" pin="VDDSHV63"/>
                                <connect gate="N" pad="G14" pin="VDDSHV8"/>
                                <connect gate="N" pad="G13" pin="VDDSHV82"/>
                                <connect gate="N" pad="G11" pin="VDDSHV9"/>
                                <connect gate="N" pad="G10" pin="VDDSHV10"/>
                                <connect gate="C" pad="F1" pin="DDR_DQSN0"/>
                                <connect gate="C" pad="F2" pin="DDR_DQS0"/>
                                <connect gate="O" pad="F3" pin="DDR_D3"/>
                                <connect gate="C" pad="F4" pin="DDR_DQM0"/>
                                <connect gate="D" pad="F6" pin="GPMC_A7"/>
                                <connect gate="D" pad="F7" pin="GPMC_A8"/>
                                <connect gate="M" pad="F8" pin="VDDS3P3V_IOLDO"/>
                                <connect gate="O" pad="AB1" pin="DDR_D29"/>
                                <connect gate="O" pad="AB2" pin="DDR_D28"/>
                                <connect gate="K" pad="AB6" pin="RESERVED3"/>
                                <connect gate="K" pad="AB7" pin="RESERVED4"/>
                                <connect gate="K" pad="AB9" pin="RESERVED5"/>
                                <connect gate="P" pad="L2" pin="DDR_A2"/>
                                <connect gate="P" pad="L1" pin="DDR_A1"/>
                                <connect gate="J" pad="L8" pin="VSS10"/>
                                <connect gate="J" pad="L9" pin="VSS11"/>
                                <connect gate="C" pad="Y1" pin="DDR_DQM3"/>
                                <connect gate="O" pad="Y3" pin="DDR_D25"/>
                                <connect gate="O" pad="Y2" pin="DDR_D24"/>
                                <connect gate="O" pad="Y4" pin="DDR_D26"/>
                                <connect gate="K" pad="Y7" pin="RESERVED6"/>
                                <connect gate="K" pad="Y6" pin="RESERVED7"/>
                                <connect gate="P" pad="R4" pin="DDR_A6"/>
                                <connect gate="P" pad="R5" pin="DDR_A5"/>
                                <connect gate="M" pad="R6" pin="VDDS_DDR3"/>
                                <connect gate="M" pad="R7" pin="VDDS_DDR4"/>
                                <connect gate="P" pad="R1" pin="DDR_A9"/>
                                <connect gate="P" pad="R2" pin="DDR_A8"/>
                                <connect gate="P" pad="R3" pin="DDR_A7"/>
                                <connect gate="M" pad="R8" pin="VDDS_DDR5"/>
                                <connect gate="Q" pad="R9" pin="VDD_CORE4"/>
                                <connect gate="J" pad="U19" pin="VSS12"/>
                                <connect gate="N" pad="W18" pin="VDDSHV32"/>
                                <connect gate="N" pad="W16" pin="VDDSHV2"/>
                                <connect gate="M" pad="W15" pin="VDDS5"/>
                                <connect gate="Q" pad="W13" pin="VDD_CORE5"/>
                                <connect gate="Q" pad="W12" pin="VDD_CORE6"/>
                                <connect gate="K" pad="W10" pin="RESERVED8"/>
                                <connect gate="J" pad="U13" pin="VSS13"/>
                                <connect gate="J" pad="U12" pin="VSS14"/>
                                <connect gate="D" pad="E8" pin="GPMC_A6"/>
                                <connect gate="D" pad="E7" pin="GPMC_A5"/>
                                <connect gate="O" pad="E1" pin="DDR_D2"/>
                                <connect gate="O" pad="E3" pin="DDR_D0"/>
                                <connect gate="O" pad="E2" pin="DDR_D1"/>
                                <connect gate="A" pad="F19" pin="CAP_VBB_MPU"/>
                                <connect gate="M" pad="F13" pin="VDDS_SRAM_CORE_BG"/>
                                <connect gate="U" pad="F10" pin="GPMC_CSN2"/>
                                <connect gate="U" pad="F11" pin="GPMC_AD10"/>
                                <connect gate="N" pad="F16" pin="VDDSHV7"/>
                                <connect gate="H" pad="F17" pin="MII1_RXD0"/>
                                <connect gate="M" pad="F14" pin="VDDS_SRAM_MPU_BB"/>
                                <connect gate="J" pad="N12" pin="VSS15"/>
                                <connect gate="J" pad="N13" pin="VSS16"/>
                                <connect gate="J" pad="N10" pin="VSS17"/>
                                <connect gate="J" pad="N11" pin="VSS18"/>
                                <connect gate="Q" pad="N16" pin="VDD_CORE7"/>
                                <connect gate="Q" pad="N17" pin="VDD_CORE8"/>
                                <connect gate="J" pad="N14" pin="VSS19"/>
                                <connect gate="J" pad="N15" pin="VSS20"/>
                                <connect gate="N" pad="N18" pin="VDDSHV33"/>
                                <connect gate="N" pad="N19" pin="VDDSHV34"/>
                                <connect gate="G" pad="P25" pin="SPI4_SCLK"/>
                                <connect gate="G" pad="P24" pin="SPI4_D1"/>
                                <connect gate="K" pad="P21" pin="RESERVED9"/>
                                <connect gate="G" pad="P20" pin="SPI2_D1"/>
                                <connect gate="G" pad="P23" pin="SPI0_SCLK"/>
                                <connect gate="G" pad="P22" pin="SPI2_D0"/>
                                <connect gate="B" pad="H25" pin="UART3_RXD"/>
                                <connect gate="B" pad="H24" pin="UART3_TXD"/>
                                <connect gate="K" pad="H21" pin="RESERVED10"/>
                                <connect gate="B" pad="H20" pin="CLKREQ"/>
                                <connect gate="B" pad="H23" pin="MCASP0_AXR0"/>
                                <connect gate="B" pad="H22" pin="UART3_CTSN"/>
                                <connect gate="C" pad="K3" pin="DDR_BA2"/>
                                <connect gate="C" pad="K2" pin="DDR_BA1"/>
                                <connect gate="C" pad="K1" pin="DDR_BA0"/>
                                <connect gate="M" pad="K7" pin="VDDS_DDR6"/>
                                <connect gate="O" pad="K6" pin="DDR_D13"/>
                                <connect gate="O" pad="K5" pin="DDR_D14"/>
                                <connect gate="O" pad="K4" pin="DDR_D15"/>
                                <connect gate="J" pad="U11" pin="VSS21"/>
                                <connect gate="J" pad="U10" pin="VSS22"/>
                                <connect gate="J" pad="K9" pin="VSS23"/>
                                <connect gate="M" pad="K8" pin="VDDS_DDR7"/>
                                <connect gate="Q" pad="U15" pin="VDD_CORE9"/>
                                <connect gate="J" pad="U14" pin="VSS24"/>
                                <connect gate="J" pad="U17" pin="VSS25"/>
                                <connect gate="J" pad="U16" pin="VSS26"/>
                                <connect gate="E" pad="AB25" pin="CAM1_WEN"/>
                                <connect gate="B" pad="AB24" pin="I2C0_SDA"/>
                                <connect gate="E" pad="AB20" pin="CAM1_DATA0"/>
                                <connect gate="J" pad="M11" pin="VSS27"/>
                                <connect gate="J" pad="M10" pin="VSS28"/>
                                <connect gate="J" pad="M13" pin="VSS29"/>
                                <connect gate="Q" pad="M12" pin="VDD_CORE10"/>
                                <connect gate="J" pad="M15" pin="VSS30"/>
                                <connect gate="Q" pad="M14" pin="VDD_CORE11"/>
                                <connect gate="L" pad="M17" pin="VDD_MPU4"/>
                                <connect gate="J" pad="M16" pin="VSS31"/>
                                <connect gate="L" pad="M18" pin="VDD_MPU5"/>
                                <connect gate="F" pad="E19" pin="DSS_DATA7"/>
                                <connect gate="U" pad="E11" pin="GPMC_AD12"/>
                                <connect gate="U" pad="E10" pin="GPMC_OEN_REN"/>
                                <connect gate="A" pad="E13" pin="CAP_VDD_SRAM_CORE"/>
                                <connect gate="A" pad="E14" pin="CAP_VDD_SRAM_MPU"/>
                                <connect gate="M" pad="E17" pin="VDDS_PLL_MPU"/>
                                <connect gate="H" pad="E16" pin="MII1_RXD2"/>
                                <connect gate="B" pad="K22" pin="UART1_CTSN"/>
                                <connect gate="B" pad="K23" pin="MCASP0_FSR"/>
                                <connect gate="L" pad="K20" pin="VDD_MPU6"/>
                                <connect gate="B" pad="K21" pin="UART1_RXD"/>
                                <connect gate="B" pad="K24" pin="UART3_RTSN"/>
                                <connect gate="B" pad="K25" pin="UART0_RXD"/>
                                <connect gate="J" pad="U18" pin="VSS32"/>
                                <connect gate="J" pad="V18" pin="VSS33"/>
                                <connect gate="J" pad="V12" pin="VSS34"/>
                                <connect gate="J" pad="V13" pin="VSS35"/>
                                <connect gate="J" pad="V10" pin="VSS36"/>
                                <connect gate="J" pad="V11" pin="VSS37"/>
                                <connect gate="N" pad="V16" pin="VDDSHV22"/>
                                <connect gate="N" pad="V17" pin="VDDSHV23"/>
                                <connect gate="J" pad="V14" pin="VSS38"/>
                                <connect gate="Q" pad="V15" pin="VDD_CORE12"/>
                                <connect gate="K" pad="AA7" pin="RESERVED11"/>
                                <connect gate="C" pad="AA1" pin="DDR_DQS3"/>
                                <connect gate="D" pad="D8" pin="GPMC_A11"/>
                                <connect gate="C" pad="AA2" pin="DDR_DQSN3"/>
                                <connect gate="A" pad="D6" pin="CAP_VDDS1P8V_IOLDO"/>
                                <connect gate="D" pad="D7" pin="GPMC_A4"/>
                                <connect gate="V" pad="D2" pin="MMC0_CMD"/>
                                <connect gate="V" pad="D1" pin="MMC0_CLK"/>
                                <connect gate="B" pad="F23" pin="GPIO5_11"/>
                                <connect gate="N" pad="F22" pin="VDDSHV5"/>
                                <connect gate="M" pad="F20" pin="VDDS6"/>
                                <connect gate="B" pad="F25" pin="USB1_DRVVBUS"/>
                                <connect gate="B" pad="F24" pin="GPIO5_9"/>
                                <connect gate="B" pad="N23" pin="EMU0"/>
                                <connect gate="B" pad="N22" pin="MCASP0_FSX"/>
                                <connect gate="M" pad="N21" pin="VDDS_PLL_CORE_LCD"/>
                                <connect gate="G" pad="N20" pin="SPI2_SCLK"/>
                                <connect gate="G" pad="N25" pin="SPI4_CS0"/>
                                <connect gate="B" pad="N24" pin="MCASP0_ACLKX"/>
                                <connect gate="M" pad="C23" pin="VDDS_OSC"/>
                                <connect gate="F" pad="C20" pin="DSS_DATA6"/>
                                <connect gate="F" pad="C21" pin="DSS_DATA3"/>
                                <connect gate="R" pad="C24" pin="XDMA_EVENT_INTR1"/>
                                <connect gate="R" pad="C25" pin="XTALIN"/>
                                <connect gate="N" pad="J8" pin="VDDSHV1"/>
                                <connect gate="J" pad="J9" pin="VSS39"/>
                                <connect gate="O" pad="J4" pin="DDR_D11"/>
                                <connect gate="O" pad="J5" pin="DDR_D10"/>
                                <connect gate="O" pad="J6" pin="DDR_D9"/>
                                <connect gate="N" pad="J7" pin="VDDSHV12"/>
                                <connect gate="C" pad="J1" pin="DDR_DQSN1"/>
                                <connect gate="C" pad="J2" pin="DDR_DQS1"/>
                                <connect gate="O" pad="J3" pin="DDR_D12"/>
                                <connect gate="O" pad="W6" pin="DDR_D23"/>
                                <connect gate="O" pad="W5" pin="DDR_D22"/>
                                <connect gate="O" pad="W4" pin="DDR_D21"/>
                                <connect gate="C" pad="W2" pin="DDR_DQSN2"/>
                                <connect gate="C" pad="W1" pin="DDR_DQS2"/>
                                <connect gate="J" pad="L18" pin="VSS40"/>
                                <connect gate="L" pad="L19" pin="VDD_MPU7"/>
                                <connect gate="Q" pad="L14" pin="VDD_CORE13"/>
                                <connect gate="J" pad="L15" pin="VSS41"/>
                                <connect gate="J" pad="L17" pin="VSS42"/>
                                <connect gate="J" pad="L11" pin="VSS43"/>
                                <connect gate="Q" pad="L12" pin="VDD_CORE14"/>
                                <connect gate="Q" pad="T14" pin="VDD_CORE15"/>
                                <connect gate="J" pad="T15" pin="VSS44"/>
                                <connect gate="J" pad="T17" pin="VSS45"/>
                                <connect gate="Q" pad="T11" pin="VDD_CORE16"/>
                                <connect gate="J" pad="T12" pin="VSS46"/>
                                <connect gate="Q" pad="T18" pin="VDD_CORE17"/>
                                <connect gate="Q" pad="T19" pin="VDD_CORE18"/>
                                <connect gate="S" pad="AC16" pin="ADC1_AIN0"/>
                                <connect gate="J" pad="AC15" pin="VSSA_ADC"/>
                                <connect gate="S" pad="AC13" pin="ADC0_AIN5"/>
                                <connect gate="K" pad="AC12" pin="RESERVED12"/>
                                <connect gate="K" pad="AC10" pin="RESERVED13"/>
                                <connect gate="E" pad="AC18" pin="CAM0_FIELD"/>
                                <connect gate="N" pad="H10" pin="VDDSHV102"/>
                                <connect gate="N" pad="H11" pin="VDDSHV92"/>
                                <connect gate="P" pad="P2" pin="DDR_A3"/>
                                <connect gate="P" pad="P1" pin="DDR_A4"/>
                                <connect gate="J" pad="P8" pin="VSS47"/>
                                <connect gate="J" pad="P9" pin="VSS48"/>
                                <connect gate="J" pad="AE1" pin="VSS49"/>
                                <connect gate="V" pad="AE3" pin="RTC_WAKEUP"/>
                                <connect gate="V" pad="AE2" pin="RTC_KALDO_ENN"/>
                                <connect gate="V" pad="AE5" pin="RTC_XTALIN"/>
                                <connect gate="V" pad="AE4" pin="RTC_XTALOUT"/>
                                <connect gate="J" pad="AE7" pin="VSS50"/>
                                <connect gate="V" pad="AE6" pin="RTC_PWRONRSTN"/>
                                <connect gate="K" pad="AE9" pin="RESERVED14"/>
                                <connect gate="J" pad="AE8" pin="VSS51"/>
                                <connect gate="J" pad="K11" pin="VSS52"/>
                                <connect gate="E" pad="AD21" pin="CAM1_DATA2"/>
                                <connect gate="E" pad="AD20" pin="CAM0_DATA7"/>
                                <connect gate="E" pad="AD23" pin="CAM1_DATA6"/>
                                <connect gate="E" pad="AD22" pin="CAM1_DATA4"/>
                                <connect gate="U" pad="D10" pin="GPMC_WEN"/>
                                <connect gate="U" pad="D11" pin="GPMC_AD11"/>
                                <connect gate="J" pad="K15" pin="VSS53"/>
                                <connect gate="H" pad="D13" pin="MII1_RX_CLK"/>
                                <connect gate="L" pad="K19" pin="VDD_MPU8"/>
                                <connect gate="N" pad="K18" pin="VDDSHV35"/>
                                <connect gate="F" pad="D19" pin="DSS_DATA13"/>
                                <connect gate="N" pad="K17" pin="VDDSHV36"/>
                                <connect gate="T" pad="V24" pin="USB1_DP"/>
                                <connect gate="U" pad="C8" pin="GPMC_AD6"/>
                                <connect gate="D" pad="C3" pin="GPMC_A0"/>
                                <connect gate="V" pad="C2" pin="MMC0_DAT1"/>
                                <connect gate="V" pad="C1" pin="MMC0_DAT0"/>
                                <connect gate="D" pad="C6" pin="GPMC_A2"/>
                                <connect gate="D" pad="C5" pin="GPMC_A1"/>
                                <connect gate="E" pad="AE19" pin="CAM0_DATA4"/>
                                <connect gate="E" pad="AE18" pin="CAM0_DATA0"/>
                                <connect gate="S" pad="AE15" pin="ADC1_VREFP"/>
                                <connect gate="S" pad="AE14" pin="ADC0_VREFN"/>
                                <connect gate="E" pad="AE17" pin="CAM0_HD"/>
                                <connect gate="S" pad="AE16" pin="ADC1_AIN6"/>
                                <connect gate="K" pad="AE11" pin="RESERVED15"/>
                                <connect gate="J" pad="AE10" pin="VSS54"/>
                                <connect gate="S" pad="AE13" pin="ADC0_AIN7"/>
                                <connect gate="K" pad="AE12" pin="RESERVED16"/>
                                <connect gate="F" pad="A20" pin="DSS_DATA4"/>
                                <connect gate="F" pad="A21" pin="DSS_DATA1"/>
                                <connect gate="F" pad="A22" pin="DSS_PCLK"/>
                                <connect gate="F" pad="A23" pin="DSS_HSYNC"/>
                                <connect gate="F" pad="A24" pin="DSS_AC_BIAS_EN"/>
                                <connect gate="J" pad="A25" pin="VSS55"/>
                                <connect gate="F" pad="C19" pin="DSS_DATA12"/>
                                <connect gate="H" pad="C13" pin="MII1_TXD2"/>
                                <connect gate="U" pad="C11" pin="GPMC_AD13"/>
                                <connect gate="U" pad="C10" pin="GPMC_BE0N_CLE"/>
                                <connect gate="F" pad="C17" pin="DSS_DATA14"/>
                                <connect gate="H" pad="C16" pin="MII1_TXD3"/>
                                <connect gate="H" pad="C14" pin="MII1_RXD3"/>
                                <connect gate="A" pad="AB12" pin="VDDA_ADC0"/>
                                <connect gate="S" pad="AB13" pin="ADC0_AIN4"/>
                                <connect gate="K" pad="AB10" pin="RESERVED17"/>
                                <connect gate="S" pad="AB16" pin="ADC1_AIN1"/>
                                <connect gate="S" pad="AB15" pin="ADC1_AIN3"/>
                                <connect gate="E" pad="AB18" pin="CAM0_DATA1"/>
                                <connect gate="E" pad="AB19" pin="CAM0_DATA8"/>
                                <connect gate="O" pad="V1" pin="DDR_D20"/>
                                <connect gate="O" pad="V2" pin="DDR_D19"/>
                                <connect gate="O" pad="V3" pin="DDR_D18"/>
                                <connect gate="O" pad="V4" pin="DDR_D17"/>
                                <connect gate="O" pad="V5" pin="DDR_D16"/>
                                <connect gate="C" pad="V6" pin="DDR_DQM2"/>
                                <connect gate="M" pad="V7" pin="VDDS_DDR8"/>
                                <connect gate="M" pad="V8" pin="VDDS_DDR9"/>
                                <connect gate="J" pad="V9" pin="VSS56"/>
                                <connect gate="H" pad="D14" pin="MII1_TX_CLK"/>
                                <connect gate="J" pad="K12" pin="VSS57"/>
                                <connect gate="H" pad="D16" pin="MII1_COL"/>
                                <connect gate="F" pad="D17" pin="DSS_DATA15"/>
                                <connect gate="G" pad="Y20" pin="TDI"/>
                                <connect gate="E" pad="AD25" pin="CAM1_HD"/>
                                <connect gate="B" pad="Y22" pin="I2C0_SCL"/>
                                <connect gate="B" pad="Y23" pin="PWRONRSTN"/>
                                <connect gate="G" pad="Y24" pin="TMS"/>
                                <connect gate="B" pad="Y25" pin="NTRST"/>
                                <connect gate="E" pad="AD24" pin="CAM1_DATA8"/>
                                <connect gate="J" pad="K14" pin="VSS58"/>
                                <connect gate="E" pad="AD18" pin="CAM0_VD"/>
                                <connect gate="E" pad="AD19" pin="CAM0_DATA5"/>
                                <connect gate="K" pad="AD10" pin="RESERVED18"/>
                                <connect gate="K" pad="AD11" pin="RESERVED19"/>
                                <connect gate="M" pad="AD12" pin="VDDS7"/>
                                <connect gate="S" pad="AD13" pin="ADC0_AIN6"/>
                                <connect gate="S" pad="AD14" pin="ADC0_VREFP"/>
                                <connect gate="S" pad="AD15" pin="ADC1_VREFN"/>
                                <connect gate="S" pad="AD16" pin="ADC1_AIN7"/>
                                <connect gate="E" pad="AD17" pin="CAM0_WEN"/>
                                <connect gate="D" pad="B4" pin="GPMC_A9"/>
                                <connect gate="U" pad="B5" pin="GPMC_AD0"/>
                                <connect gate="U" pad="B6" pin="GPMC_AD2"/>
                                <connect gate="U" pad="B7" pin="GPMC_AD4"/>
                                <connect gate="V" pad="B1" pin="MMC0_DAT3"/>
                                <connect gate="V" pad="B2" pin="MMC0_DAT2"/>
                                <connect gate="D" pad="B3" pin="GPMC_WPN"/>
                                <connect gate="U" pad="B8" pin="GPMC_AD7"/>
                                <connect gate="U" pad="B9" pin="GPMC_CSN1"/>
                                <connect gate="J" pad="U9" pin="VSS59"/>
                                <connect gate="J" pad="U8" pin="VSS60"/>
                                <connect gate="C" pad="U1" pin="DDR_ODT0"/>
                                <connect gate="C" pad="U2" pin="DDR_ODT1"/>
                                <connect gate="E" pad="AE24" pin="CAM1_DATA7"/>
                                <connect gate="J" pad="AE25" pin="VSS61"/>
                                <connect gate="E" pad="AE20" pin="CAM0_DATA6"/>
                                <connect gate="E" pad="AE21" pin="CAM1_PCLK"/>
                                <connect gate="E" pad="AE22" pin="CAM1_DATA3"/>
                                <connect gate="E" pad="AE23" pin="CAM1_DATA5"/>
                                <connect gate="J" pad="R17" pin="VSS62"/>
                                <connect gate="Q" pad="R14" pin="VDD_CORE19"/>
                                <connect gate="J" pad="R15" pin="VSS63"/>
                                <connect gate="J" pad="R12" pin="VSS64"/>
                                <connect gate="Q" pad="R11" pin="VDD_CORE20"/>
                                <connect gate="J" pad="R18" pin="VSS65"/>
                                <connect gate="G" pad="T21" pin="SPI0_D1"/>
                                <connect gate="B" pad="T20" pin="SPI0_CS0"/>
                                <connect gate="G" pad="T23" pin="SPI2_CS0"/>
                                <connect gate="G" pad="T22" pin="SPI0_D0"/>
                                <connect gate="T" pad="T25" pin="USB1_VBUS"/>
                                <connect gate="B" pad="T24" pin="EMU1"/>
                                <connect gate="E" pad="AC23" pin="CAM1_VD"/>
                                <connect gate="N" pad="H8" pin="VDDSHV112"/>
                                <connect gate="E" pad="AC21" pin="CAM1_DATA1"/>
                                <connect gate="T" pad="V25" pin="USB1_DM"/>
                                <connect gate="E" pad="AC24" pin="CAM1_DATA9"/>
                                <connect gate="E" pad="AC25" pin="CAM1_FIELD"/>
                                <connect gate="C" pad="H2" pin="DDR_DQM1"/>
                                <connect gate="O" pad="H1" pin="DDR_D8"/>
                                <connect gate="H" pad="B16" pin="MII1_RXD1"/>
                                <connect gate="R" pad="B17" pin="MDIO_CLK"/>
                                <connect gate="H" pad="B14" pin="MII1_CRS"/>
                                <connect gate="H" pad="B15" pin="MII1_TXD0"/>
                                <connect gate="U" pad="B12" pin="GPMC_CSN3"/>
                                <connect gate="H" pad="B13" pin="MII1_RX_ER"/>
                                <connect gate="U" pad="B10" pin="GPMC_AD8"/>
                                <connect gate="U" pad="B11" pin="GPMC_AD14"/>
                                <connect gate="F" pad="B18" pin="DSS_DATA11"/>
                                <connect gate="F" pad="B19" pin="DSS_DATA9"/>
                                <connect gate="V" pad="AD6" pin="RTC_PMIC_EN"/>
                                <connect gate="K" pad="AD7" pin="RESERVED20"/>
                                <connect gate="J" pad="AD4" pin="VSS_RTC"/>
                                <connect gate="M" pad="AD5" pin="VDDS_RTC"/>
                                <connect gate="K" pad="AD2" pin="RESERVED21"/>
                                <connect gate="A" pad="AD3" pin="CAP_VDD_RTC"/>
                                <connect gate="K" pad="AD1" pin="RESERVED22"/>
                                <connect gate="M" pad="AD8" pin="VDDS8"/>
                                <connect gate="Q" pad="AD9" pin="VDD_CORE21"/>
                                <connect gate="B" pad="L21" pin="UART1_TXD"/>
                                <connect gate="L" pad="L20" pin="VDD_MPU9"/>
                                <connect gate="B" pad="L23" pin="MCASP0_ACLKR"/>
                                <connect gate="B" pad="L22" pin="UART1_RTSN"/>
                                <connect gate="B" pad="L25" pin="UART0_CTSN"/>
                                <connect gate="B" pad="L24" pin="MCASP0_AHCLKX"/>
                                <connect gate="N" pad="J18" pin="VDDSHV37"/>
                                <connect gate="L" pad="J16" pin="VDD_MPU10"/>
                                <connect gate="J" pad="J17" pin="VSS66"/>
                                <connect gate="L" pad="J14" pin="VDD_MPU11"/>
                                <connect gate="J" pad="J15" pin="VSS67"/>
                                <connect gate="J" pad="J12" pin="VSS68"/>
                                <connect gate="L" pad="J13" pin="VDD_MPU12"/>
                                <connect gate="Q" pad="J10" pin="VDD_CORE22"/>
                                <connect gate="Q" pad="J11" pin="VDD_CORE23"/>
                                <connect gate="L" pad="D20" pin="VDD_MPU_MON"/>
                                <connect gate="B" pad="D25" pin="GPIO5_8"/>
                                <connect gate="R" pad="D24" pin="XDMA_EVENT_INTR0"/>
                                <connect gate="M" pad="N8" pin="VDDS_DDR10"/>
                                <connect gate="Q" pad="N9" pin="VDD_CORE24"/>
                                <connect gate="P" pad="N1" pin="DDR_A0"/>
                                <connect gate="C" pad="N2" pin="DDR_RASN"/>
                                <connect gate="C" pad="N3" pin="DDR_CASN"/>
                                <connect gate="C" pad="N4" pin="DDR_WEN"/>
                                <connect gate="P" pad="N5" pin="DDR_A13"/>
                                <connect gate="C" pad="N6" pin="DDR_CKE1"/>
                                <connect gate="M" pad="N7" pin="VDDS_DDR11"/>
                                <connect gate="C" pad="AC3" pin="DDR_VTP"/>
                                <connect gate="O" pad="AC2" pin="DDR_D31"/>
                                <connect gate="O" pad="AC1" pin="DDR_D30"/>
                                <connect gate="K" pad="AC7" pin="RESERVED23"/>
                                <connect gate="K" pad="AC6" pin="RESERVED24"/>
                                <connect gate="K" pad="AC5" pin="RESERVED25"/>
                                <connect gate="K" pad="AC9" pin="RESERVED26"/>
                                <connect gate="K" pad="AA10" pin="RESERVED27"/>
                                <connect gate="S" pad="AA13" pin="ADC0_AIN3"/>
                                <connect gate="S" pad="AA15" pin="ADC1_AIN4"/>
                                <connect gate="S" pad="AA16" pin="ADC1_AIN2"/>
                                <connect gate="E" pad="AA19" pin="CAM0_DATA9"/>
                                <connect gate="E" pad="AA18" pin="CAM0_DATA3"/>
                                <connect gate="H" pad="A15" pin="MII1_RX_DV"/>
                                <connect gate="H" pad="A14" pin="MII1_TXD1"/>
                                <connect gate="R" pad="A17" pin="MDIO_DATA"/>
                                <connect gate="H" pad="A16" pin="RMII1_REF_CLK"/>
                                <connect gate="U" pad="A11" pin="GPMC_AD15"/>
                                <connect gate="U" pad="A10" pin="GPMC_AD9"/>
                                <connect gate="H" pad="A13" pin="MII1_TX_EN"/>
                                <connect gate="U" pad="A12" pin="GPMC_CLK"/>
                                <connect gate="F" pad="A19" pin="DSS_DATA8"/>
                                <connect gate="F" pad="A18" pin="DSS_DATA10"/>
                                <connect gate="J" pad="A1" pin="VSS69"/>
                                <connect gate="D" pad="A3" pin="GPMC_BE1N"/>
                                <connect gate="D" pad="A2" pin="GPMC_WAIT0"/>
                                <connect gate="U" pad="A5" pin="GPMC_AD1"/>
                                <connect gate="D" pad="A4" pin="GPMC_A3"/>
                                <connect gate="U" pad="A7" pin="GPMC_AD5"/>
                                <connect gate="U" pad="A6" pin="GPMC_AD3"/>
                                <connect gate="U" pad="A9" pin="GPMC_ADVN_ALE"/>
                                <connect gate="U" pad="A8" pin="GPMC_CSN0"/>
                                <connect gate="O" pad="AA3" pin="DDR_D27"/>
                                <connect gate="M" pad="T8" pin="VDDS_DDR12"/>
                                <connect gate="Q" pad="T9" pin="VDD_CORE25"/>
                                <connect gate="C" pad="T6" pin="DDR_VREF"/>
                                <connect gate="M" pad="T7" pin="VDDS_DDR13"/>
                                <connect gate="P" pad="T4" pin="DDR_A12"/>
                                <connect gate="P" pad="T5" pin="DDR_A11"/>
                                <connect gate="P" pad="T2" pin="DDR_A15"/>
                                <connect gate="P" pad="T3" pin="DDR_A14"/>
                                <connect gate="C" pad="T1" pin="DDR_RESETN"/>
                                <connect gate="K" pad="AA9" pin="RESERVED28"/>
                                <connect gate="G" pad="R25" pin="SPI0_CS1"/>
                                <connect gate="G" pad="R24" pin="SPI4_D0"/>
                                <connect gate="S" pad="AA12" pin="ADC0_AIN0"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="595-AM4376BZDN100"/>
                                    <attribute name="temperature_range_high" value="+90°C"/>
                                    <attribute name="MPN" value="AM4376BZDN100"/>
                                    <attribute name="digikey_description" value="IC ARM® Cortex®-A9 Microprocessor IC Sitara™ 1 Core, 32-Bit 1.0GHz 491-NFBGA (17x17)"/>
                                    <attribute name="digikey_part_number" value="296-42747-ND"/>
                                    <attribute name="prefix" value="U"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="mfg_package_ident" value="ZDN (S-PBGA-N491)"/>
                                    <attribute name="voltage" value=""/>
                                    <attribute name="temperature_range_low" value="0°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="datasheet" value="http://www.ti.com/lit/ds/symlink/am4376.pdf"/>
                                    <attribute name="centroid_not_specified" value=""/>
                                    <attribute name="MF" value="Texas Instruments"/>
                                    <attribute name="package" value="NFBGA491"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="U" name="ANALOG_DEVICES_INC._ADV7180BSTZ">
                    <description></description>
                    <gates>
                        <gate name="B" symbol="ANALOG_DEVICES_INC._ADV7180BSTZ_0_0"/>
                        <gate name="A" symbol="ANALOG_DEVICES_INC._ADV7180BSTZ_0_1"/>
                    </gates>
                    <devices>
                        <device name="ANALOG_DEVICES_INC._ADV7180BSTZ_0_0" package="ANALOG_DEVICES_INC._ADV7180BSTZ_0">
                            <connects>
                                <connect gate="B" pad="1" pin="!INTRQ"/>
                                <connect gate="B" pad="2" pin="HS"/>
                                <connect gate="A" pad="3" pin="DGND"/>
                                <connect gate="A" pad="4" pin="DVDDIO"/>
                                <connect gate="B" pad="5" pin="P11"/>
                                <connect gate="B" pad="6" pin="P10"/>
                                <connect gate="B" pad="7" pin="P9"/>
                                <connect gate="B" pad="8" pin="P8"/>
                                <connect gate="B" pad="9" pin="SFL"/>
                                <connect gate="A" pad="10" pin="DGND2"/>
                                <connect gate="A" pad="11" pin="DVDDIO2"/>
                                <connect gate="B" pad="12" pin="GPO1"/>
                                <connect gate="B" pad="13" pin="GPO0"/>
                                <connect gate="B" pad="14" pin="P7"/>
                                <connect gate="B" pad="15" pin="P6"/>
                                <connect gate="B" pad="16" pin="P5"/>
                                <connect gate="B" pad="17" pin="P4"/>
                                <connect gate="B" pad="18" pin="P3"/>
                                <connect gate="B" pad="19" pin="P2"/>
                                <connect gate="B" pad="20" pin="LLC"/>
                                <connect gate="B" pad="21" pin="XTAL1"/>
                                <connect gate="B" pad="22" pin="XTAL"/>
                                <connect gate="A" pad="23" pin="DVDD"/>
                                <connect gate="A" pad="24" pin="DGND3"/>
                                <connect gate="B" pad="25" pin="P1"/>
                                <connect gate="B" pad="26" pin="P0"/>
                                <connect gate="A" pad="27" pin="NC"/>
                                <connect gate="A" pad="28" pin="NC2"/>
                                <connect gate="B" pad="29" pin="!PWRDWN"/>
                                <connect gate="B" pad="30" pin="ELPF"/>
                                <connect gate="A" pad="31" pin="PVDD"/>
                                <connect gate="A" pad="32" pin="AGND"/>
                                <connect gate="A" pad="33" pin="NC3"/>
                                <connect gate="B" pad="34" pin="TEST_0"/>
                                <connect gate="B" pad="35" pin="AIN1"/>
                                <connect gate="B" pad="36" pin="AIN2"/>
                                <connect gate="A" pad="37" pin="AGND2"/>
                                <connect gate="B" pad="38" pin="VREFP"/>
                                <connect gate="B" pad="39" pin="VREFN"/>
                                <connect gate="A" pad="40" pin="AVDD"/>
                                <connect gate="A" pad="41" pin="NC4"/>
                                <connect gate="A" pad="42" pin="NC5"/>
                                <connect gate="A" pad="43" pin="AGND3"/>
                                <connect gate="A" pad="44" pin="NC6"/>
                                <connect gate="A" pad="45" pin="NC7"/>
                                <connect gate="B" pad="46" pin="AIN3"/>
                                <connect gate="B" pad="47" pin="AIN4"/>
                                <connect gate="B" pad="48" pin="AIN5"/>
                                <connect gate="B" pad="49" pin="AIN6"/>
                                <connect gate="A" pad="50" pin="NC8"/>
                                <connect gate="B" pad="51" pin="!RESET"/>
                                <connect gate="B" pad="52" pin="ALSB"/>
                                <connect gate="B" pad="53" pin="SDATA"/>
                                <connect gate="B" pad="54" pin="SCLK"/>
                                <connect gate="B" pad="55" pin="GPO3"/>
                                <connect gate="B" pad="56" pin="GPO2"/>
                                <connect gate="A" pad="57" pin="DGND4"/>
                                <connect gate="A" pad="58" pin="DVDD2"/>
                                <connect gate="B" pad="59" pin="P15"/>
                                <connect gate="B" pad="60" pin="P14"/>
                                <connect gate="B" pad="61" pin="P13"/>
                                <connect gate="B" pad="62" pin="P12"/>
                                <connect gate="B" pad="63" pin="FIELD"/>
                                <connect gate="B" pad="64" pin="VS"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="584-ADV7180BSTZ-R"/>
                                    <attribute name="temperature_range_high" value="+85°C"/>
                                    <attribute name="temperature_range_low" value="-40°C"/>
                                    <attribute name="digikey_part_number" value="ADV7180BSTZ-REELCT-ND"/>
                                    <attribute name="MF" value="Analog Devices Inc."/>
                                    <attribute name="datasheet" value="http://media.digikey.com/pdf/Data%20Sheets/Analog%20Devices%20PDFs/ADV7180.pdf"/>
                                    <attribute name="MPN" value="ADV7180BSTZ"/>
                                    <attribute name="mfg_package_ident" value=""/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="digikey_description" value="IC VIDEO DECODER SDTV 64-LQFP"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="prefix" value="U"/>
                                    <attribute name="ipc_land_pattern_name" value="QFP50P1200X1200X160-64"/>
                                    <attribute name="package" value="LQFP64"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="U" name="TEXAS_INSTRUMENTS_TPS65218B1RSLT">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="TEXAS_INSTRUMENTS_TPS65218B1RSLT_0_0"/>
                    </gates>
                    <devices>
                        <device name="TEXAS_INSTRUMENTS_TPS65218B1RSLT_0_0" package="TEXAS_INSTRUMENTS_TPS65218B1RSLT_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="IN_DCDC1"/>
                                <connect gate="G$0" pad="2" pin="SDA"/>
                                <connect gate="G$0" pad="3" pin="SCL"/>
                                <connect gate="G$0" pad="4" pin="LD01"/>
                                <connect gate="G$0" pad="5" pin="IN_LD01"/>
                                <connect gate="G$0" pad="6" pin="IN_LS3"/>
                                <connect gate="G$0" pad="7" pin="LS3"/>
                                <connect gate="G$0" pad="8" pin="PGOOD"/>
                                <connect gate="G$0" pad="9" pin="AC_DET"/>
                                <connect gate="G$0" pad="10" pin="!PFO"/>
                                <connect gate="G$0" pad="11" pin="GPIO1"/>
                                <connect gate="G$0" pad="12" pin="IN_DCDC4"/>
                                <connect gate="G$0" pad="13" pin="L4A"/>
                                <connect gate="G$0" pad="14" pin="L4B"/>
                                <connect gate="G$0" pad="15" pin="DCDC4"/>
                                <connect gate="G$0" pad="16" pin="PFI"/>
                                <connect gate="G$0" pad="17" pin="DC34_SEL"/>
                                <connect gate="G$0" pad="18" pin="IN_NCC"/>
                                <connect gate="G$0" pad="19" pin="PGOOD_BU"/>
                                <connect gate="G$0" pad="20" pin="L5"/>
                                <connect gate="G$0" pad="21" pin="FB5"/>
                                <connect gate="G$0" pad="22" pin="FB6"/>
                                <connect gate="G$0" pad="23" pin="L6"/>
                                <connect gate="G$0" pad="24" pin="SYS_BU"/>
                                <connect gate="G$0" pad="25" pin="CC"/>
                                <connect gate="G$0" pad="26" pin="GPIO3"/>
                                <connect gate="G$0" pad="27" pin="IN_BU"/>
                                <connect gate="G$0" pad="28" pin="NC"/>
                                <connect gate="G$0" pad="29" pin="NC2"/>
                                <connect gate="G$0" pad="30" pin="LS1"/>
                                <connect gate="G$0" pad="31" pin="IN_LS1"/>
                                <connect gate="G$0" pad="32" pin="IN_LS2"/>
                                <connect gate="G$0" pad="33" pin="LS2"/>
                                <connect gate="G$0" pad="34" pin="GPO2"/>
                                <connect gate="G$0" pad="35" pin="INT_LDO"/>
                                <connect gate="G$0" pad="36" pin="IN_BIAS"/>
                                <connect gate="G$0" pad="37" pin="IN_DCDC3"/>
                                <connect gate="G$0" pad="38" pin="L3"/>
                                <connect gate="G$0" pad="39" pin="FB3"/>
                                <connect gate="G$0" pad="40" pin="!WAKEUP"/>
                                <connect gate="G$0" pad="41" pin="FB2"/>
                                <connect gate="G$0" pad="42" pin="L2"/>
                                <connect gate="G$0" pad="43" pin="IN_DCDC2"/>
                                <connect gate="G$0" pad="44" pin="PB"/>
                                <connect gate="G$0" pad="45" pin="!INT"/>
                                <connect gate="G$0" pad="46" pin="PWR_EN"/>
                                <connect gate="G$0" pad="47" pin="FB1"/>
                                <connect gate="G$0" pad="48" pin="L1"/>
                                <connect gate="G$0" pad="49-10 49-11 49-16 49 49-17 49-2 49-3 49-12 49-13 49-6 49-7 49-4 49-5 49-14 49-8 49-9 49-15" pin="GND_PAD"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="595-TPS65218B1RSLT"/>
                                    <attribute name="temperature_range_high" value="+125°C"/>
                                    <attribute name="digikey_description" value="IC REG ARM A8/A9 SOC 48VQFN"/>
                                    <attribute name="digikey_part_number" value="296-38611-1-ND"/>
                                    <attribute name="datasheet" value="http://www.ti.com/lit/ds/symlink/tps65218.pdf"/>
                                    <attribute name="MPN" value="TPS65218B1RSLT"/>
                                    <attribute name="mfg_package_ident" value="RSL (S-PVQFN-N48)"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="temperature_range_low" value="-40°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="prefix" value="U"/>
                                    <attribute name="MF" value="Texas Instruments"/>
                                    <attribute name="package" value="VQFN48"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="U" name="TEXAS_INSTRUMENTS_TPS62160DSGR">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="TEXAS_INSTRUMENTS_TPS62160DSGR_0_0"/>
                    </gates>
                    <devices>
                        <device name="TEXAS_INSTRUMENTS_TPS62160DSGR_0_0" package="TEXAS_INSTRUMENTS_TPS62160DSGR_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="PGND"/>
                                <connect gate="G$0" pad="2" pin="VIN"/>
                                <connect gate="G$0" pad="3" pin="EN"/>
                                <connect gate="G$0" pad="4" pin="AGND"/>
                                <connect gate="G$0" pad="5" pin="FB"/>
                                <connect gate="G$0" pad="6" pin="VOS"/>
                                <connect gate="G$0" pad="7" pin="SW"/>
                                <connect gate="G$0" pad="8" pin="PG"/>
                                <connect gate="G$0" pad="9" pin="AGND_PAD"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="595-TPS62160DSGR"/>
                                    <attribute name="temperature_range_high" value="+85°C"/>
                                    <attribute name="MPN" value="TPS62160DSGR"/>
                                    <attribute name="digikey_description" value="IC Buck Switching Regulator IC Positive Adjustable 0.9V 1 Output 1A 8-WFDFN Exposed Pad"/>
                                    <attribute name="digikey_part_number" value="296-29895-1-ND"/>
                                    <attribute name="prefix" value="U"/>
                                    <attribute name="datasheet" value="http://www.ti.com/lit/ds/symlink/tps62160.pdf"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="mfg_package_ident" value="DSG (S-PWSON-N8)"/>
                                    <attribute name="temperature_range_low" value="-40°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="centroid_not_specified" value=""/>
                                    <attribute name="MF" value="Texas Instruments"/>
                                    <attribute name="package" value="WSON-8"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="J" name="JST_SM02B-SRSS-TB_LF_SN">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="JST_SM02B-SRSS-TB_LF_SN_0_0"/>
                    </gates>
                    <devices>
                        <device name="JST_SM02B-SRSS-TB_LF_SN_0_0" package="JST_SM02B-SRSS-TB_LF_SN_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="1"/>
                                <connect gate="G$0" pad="2" pin="2"/>
                                <connect gate="G$0" pad="3" pin="MNT_1"/>
                                <connect gate="G$0" pad="4" pin="MNT_2"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="description" value=""/>
                                    <attribute name="temperature_range_high" value="+85ºC"/>
                                    <attribute name="MPN" value="SM02B-SRSS-TB(LF)(SN)"/>
                                    <attribute name="temperature_range_low" value="-25ºC"/>
                                    <attribute name="digikey_part_number" value="455-1802-1-ND"/>
                                    <attribute name="prefix" value="J"/>
                                    <attribute name="datasheet" value="https://upverter.com/datasheet/9acd0917c69eeea8a72691d5ce111b56ecac2c3f.pdf"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="Contact_Finish" value="Tin"/>
                                    <attribute name="digikey_description" value='CONN 2 Positions Header, Shrouded Connector 0.039" (1.00mm) Surface Mount, Right Angle Tin'/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="Current_Ratingq" value="1.0 A"/>
                                    <attribute name="MF" value="JST"/>
                                    <attribute name="Pitch" value="1.00mm"/>
                                    <attribute name="package" value="HDR02"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="U" name="TEXAS_INSTRUMENTS_LMP7702MA">
                    <description></description>
                    <gates>
                        <gate name="A" symbol="TEXAS_INSTRUMENTS_LMP7702MA_0_0"/>
                        <gate name="B" symbol="TEXAS_INSTRUMENTS_LMP7702MA_0_1"/>
                    </gates>
                    <devices>
                        <device name="TEXAS_INSTRUMENTS_LMP7702MA_0_0" package="TEXAS_INSTRUMENTS_LMP7702MA_0">
                            <connects>
                                <connect gate="A" pad="1" pin="OUT_A"/>
                                <connect gate="A" pad="2" pin="IN_A–"/>
                                <connect gate="A" pad="3" pin="IN_A+"/>
                                <connect gate="A" pad="4" pin="V–"/>
                                <connect gate="B" pad="5" pin="IN_B+"/>
                                <connect gate="B" pad="6" pin="IN_B–"/>
                                <connect gate="B" pad="7" pin="OUT_B"/>
                                <connect gate="A" pad="8" pin="V+"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="926-LMP7702MA/NOPB"/>
                                    <attribute name="prefix" value="U"/>
                                    <attribute name="ipc_land_pattern_name" value="SOIC127P600X155-8"/>
                                    <attribute name="temperature_range_high" value="+125°C"/>
                                    <attribute name="MPN" value="LMP7702MA"/>
                                    <attribute name="digikey_description" value="IC General Purpose Amplifier 2 Circuit Rail-to-Rail 8-SOIC"/>
                                    <attribute name="digikey_part_number" value="296-35343-1-ND"/>
                                    <attribute name="datasheet" value="http://www.ti.com/lit/ds/symlink/lmp7702.pdf"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="mfg_package_ident" value="D (R-PDSO-G8)"/>
                                    <attribute name="voltage" value=""/>
                                    <attribute name="temperature_range_low" value="-40°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="centroid_not_specified" value=""/>
                                    <attribute name="MF" value="Texas Instruments"/>
                                    <attribute name="package" value="8SOIC"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="U" name="VISHAY_SIA519EDJ-T1-GE3">
                    <description>Mosfet Array N and P-Channel 20V 4.5A 7.8W Surface Mount PowerPAK® SC-70-6 Dual</description>
                    <gates>
                        <gate name="A" symbol="VISHAY_SIA519EDJ-T1-GE3_0_0"/>
                        <gate name="B" symbol="VISHAY_SIA519EDJ-T1-GE3_0_1"/>
                    </gates>
                    <devices>
                        <device name="VISHAY_SIA519EDJ-T1-GE3_0_0" package="VISHAY_SIA519EDJ-T1-GE3_0">
                            <connects>
                                <connect gate="A" pad="1" pin="S1"/>
                                <connect gate="A" pad="2" pin="G1"/>
                                <connect gate="B" pad="3" pin="D2"/>
                                <connect gate="B" pad="4" pin="S2"/>
                                <connect gate="B" pad="5" pin="G2"/>
                                <connect gate="A" pad="6" pin="D1"/>
                                <connect gate="A" pad="7" pin="D12"/>
                                <connect gate="B" pad="8" pin="D22"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="781-SIA519EDJ-T1-GE3"/>
                                    <attribute name="description" value="Mosfet Array N and P-Channel 20V 4.5A 7.8W Surface Mount PowerPAK® SC-70-6 Dual"/>
                                    <attribute name="temperature_range_high" value="+150°C"/>
                                    <attribute name="MPN" value="SIA519EDJ-T1-GE3"/>
                                    <attribute name="digikey_description" value="IC Mosfet Array N and P-Channel 20V 4.5A 7.8W Surface Mount PowerPAK® SC-70-6 Dual"/>
                                    <attribute name="digikey_part_number" value="SIA519EDJ-T1-GE3CT-ND"/>
                                    <attribute name="prefix" value="U"/>
                                    <attribute name="resistance" value=""/>
                                    <attribute name="datasheet" value="http://www.vishay.com/docs/65176/sia519edj.pdf"/>
                                    <attribute name="inductance" value=""/>
                                    <attribute name="approved_alternate_part_number" value=""/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="mfg_package_ident" value=""/>
                                    <attribute name="voltage" value=""/>
                                    <attribute name="temperature_range_low" value="-55°C"/>
                                    <attribute name="capacitance" value=""/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="package" value="PowerPAK SC-70-6 Dual"/>
                                    <attribute name="octopart_part_number" value=""/>
                                    <attribute name="MF" value="Vishay"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
                <deviceset prefix="U" name="MICRON_TECHNOLOGY_INC._MT29F256G08CMCABH2-12Z">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="MICRON_TECHNOLOGY_INC._MT29F256G08CMCABH2-12Z_0_0"/>
                    </gates>
                    <devices>
                        <device name="MICRON_TECHNOLOGY_INC._MT29F256G08CMCABH2-12Z_0_0" package="MICRON_TECHNOLOGY_INC._MT29F256G08CMCABH2-12Z_0">
                            <connects>
                                <connect gate="G$0" pad="A1" pin="NC"/>
                                <connect gate="G$0" pad="A2" pin="NC2"/>
                                <connect gate="G$0" pad="A9" pin="NC3"/>
                                <connect gate="G$0" pad="A10" pin="NC4"/>
                                <connect gate="G$0" pad="B1" pin="NC5"/>
                                <connect gate="G$0" pad="B10" pin="NC6"/>
                                <connect gate="G$0" pad="D2" pin="RFU"/>
                                <connect gate="G$0" pad="D3" pin="DNU"/>
                                <connect gate="G$0" pad="D4" pin="NC7"/>
                                <connect gate="G$0" pad="D5" pin="!WP-2"/>
                                <connect gate="G$0" pad="D6" pin="NC8"/>
                                <connect gate="G$0" pad="D7" pin="NC9"/>
                                <connect gate="G$0" pad="D8" pin="DNU2"/>
                                <connect gate="G$0" pad="D9" pin="RFU2"/>
                                <connect gate="G$0" pad="E2" pin="RFU3"/>
                                <connect gate="G$0" pad="E3" pin="DNU3"/>
                                <connect gate="G$0" pad="E4" pin="NC10"/>
                                <connect gate="G$0" pad="E5" pin="!WP-1"/>
                                <connect gate="G$0" pad="E6" pin="NC11"/>
                                <connect gate="G$0" pad="E7" pin="NC12"/>
                                <connect gate="G$0" pad="E8" pin="DNU4"/>
                                <connect gate="G$0" pad="E9" pin="RFU4"/>
                                <connect gate="G$0" pad="F2" pin="VCC"/>
                                <connect gate="G$0" pad="F3" pin="VCC2"/>
                                <connect gate="G$0" pad="F4" pin="VCC3"/>
                                <connect gate="G$0" pad="F5" pin="VCC4"/>
                                <connect gate="G$0" pad="F6" pin="VCC5"/>
                                <connect gate="G$0" pad="F7" pin="VCC6"/>
                                <connect gate="G$0" pad="F8" pin="VCC7"/>
                                <connect gate="G$0" pad="F9" pin="VCC8"/>
                                <connect gate="G$0" pad="G2" pin="VSS"/>
                                <connect gate="G$0" pad="G3" pin="VSS2"/>
                                <connect gate="G$0" pad="G4" pin="VSS3"/>
                                <connect gate="G$0" pad="G5" pin="VSS4"/>
                                <connect gate="G$0" pad="G6" pin="VSS5"/>
                                <connect gate="G$0" pad="G7" pin="VSS6"/>
                                <connect gate="G$0" pad="G8" pin="VSS7"/>
                                <connect gate="G$0" pad="G9" pin="VSS8"/>
                                <connect gate="G$0" pad="H2" pin="VSSQ"/>
                                <connect gate="G$0" pad="H3" pin="VCCQ"/>
                                <connect gate="G$0" pad="H4" pin="RFU5"/>
                                <connect gate="G$0" pad="H5" pin="RFU6"/>
                                <connect gate="G$0" pad="H6" pin="R/!B2"/>
                                <connect gate="G$0" pad="H7" pin="R/!B4"/>
                                <connect gate="G$0" pad="H8" pin="VCCQ2"/>
                                <connect gate="G$0" pad="H9" pin="VSSQ2"/>
                                <connect gate="G$0" pad="J2" pin="DQ0-2"/>
                                <connect gate="G$0" pad="J3" pin="DQ2-2"/>
                                <connect gate="G$0" pad="J4" pin="ALE-2"/>
                                <connect gate="G$0" pad="J5" pin="!CE4"/>
                                <connect gate="G$0" pad="J6" pin="R/!B"/>
                                <connect gate="G$0" pad="J7" pin="R/!B3"/>
                                <connect gate="G$0" pad="J8" pin="DQ5-2"/>
                                <connect gate="G$0" pad="J9" pin="DQ7-2"/>
                                <connect gate="G$0" pad="K2" pin="DQ0-1"/>
                                <connect gate="G$0" pad="K3" pin="DQ2-1"/>
                                <connect gate="G$0" pad="K4" pin="ALE-1"/>
                                <connect gate="G$0" pad="K5" pin="!CE3"/>
                                <connect gate="G$0" pad="K6" pin="!CE2"/>
                                <connect gate="G$0" pad="K7" pin="!CE"/>
                                <connect gate="G$0" pad="K8" pin="DQ5-1"/>
                                <connect gate="G$0" pad="K9" pin="DQ7-1"/>
                                <connect gate="G$0" pad="L2" pin="VCCQ3"/>
                                <connect gate="G$0" pad="L3" pin="VSSQ3"/>
                                <connect gate="G$0" pad="L4" pin="VCCQ4"/>
                                <connect gate="G$0" pad="L5" pin="CLE-2"/>
                                <connect gate="G$0" pad="L6" pin="!RE-2(W/!R-2)"/>
                                <connect gate="G$0" pad="L7" pin="VCCQ5"/>
                                <connect gate="G$0" pad="L8" pin="VSSQ4"/>
                                <connect gate="G$0" pad="L9" pin="VCCQ6"/>
                                <connect gate="G$0" pad="M2" pin="DQ1-2"/>
                                <connect gate="G$0" pad="M3" pin="DQ3-2"/>
                                <connect gate="G$0" pad="M4" pin="VSSQ5"/>
                                <connect gate="G$0" pad="M5" pin="CLE-1"/>
                                <connect gate="G$0" pad="M6" pin="!RE-1(W/!R-1)"/>
                                <connect gate="G$0" pad="M7" pin="VSSQ6"/>
                                <connect gate="G$0" pad="M8" pin="DQ4-2"/>
                                <connect gate="G$0" pad="M9" pin="DQ6-2"/>
                                <connect gate="G$0" pad="N2" pin="DQ1-1"/>
                                <connect gate="G$0" pad="N3" pin="DQ3-1"/>
                                <connect gate="G$0" pad="N4" pin="RFU7"/>
                                <connect gate="G$0" pad="N5" pin="N/A(DQS-2)"/>
                                <connect gate="G$0" pad="N6" pin="RFU8"/>
                                <connect gate="G$0" pad="N7" pin="!WE-2(CLK-2)"/>
                                <connect gate="G$0" pad="N8" pin="DQ4-1"/>
                                <connect gate="G$0" pad="N9" pin="DQ6-1"/>
                                <connect gate="G$0" pad="P2" pin="VSSQ7"/>
                                <connect gate="G$0" pad="P3" pin="VCCQ7"/>
                                <connect gate="G$0" pad="P4" pin="RFU9"/>
                                <connect gate="G$0" pad="P5" pin="N/A(DQS-1)"/>
                                <connect gate="G$0" pad="P6" pin="RFU10"/>
                                <connect gate="G$0" pad="P7" pin="!WE-1(CLK-1)"/>
                                <connect gate="G$0" pad="P8" pin="VCCQ8"/>
                                <connect gate="G$0" pad="P9" pin="VSSQ8"/>
                                <connect gate="G$0" pad="T1" pin="NC13"/>
                                <connect gate="G$0" pad="T10" pin="NC14"/>
                                <connect gate="G$0" pad="U1" pin="NC15"/>
                                <connect gate="G$0" pad="U2" pin="NC16"/>
                                <connect gate="G$0" pad="U9" pin="NC17"/>
                                <connect gate="G$0" pad="U10" pin="NC18"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="ipc_land_pattern_name" value="BGA170N100P10X17_1800X1200X85"/>
                                    <attribute name="Memory_Size" value="256Gb (32G x 8)"/>
                                    <attribute name="MPN" value="MT29F256G08CMCABH2-12Z"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="temperature_range_high" value="+70°C"/>
                                    <attribute name="digikey_description" value="IC FLASH 256GBIT 83MHZ 100TBGA"/>
                                    <attribute name="Interface" value="Parallel"/>
                                    <attribute name="Voltage_-_Supply" value="2.7 V ~ 3.6 V"/>
                                    <attribute name="mfg_package_ident" value="100-Ball TBGA (Package Code H2)"/>
                                    <attribute name="digikey_part_number" value="MT29F256G08CMCABH2-12Z:A TR-ND"/>
                                    <attribute name="MF" value="Micron Technology Inc."/>
                                    <attribute name="prefix" value="U"/>
                                    <attribute name="datasheet" value="https://forum.upverter.com/uploads/default/original/2X/0/05fcfe4d53546abd3493a0339ace21b545f01fe5.pdf"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="Memory_Type" value="Non-Volatile"/>
                                    <attribute name="temperature_range_low" value="0°C"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="voltage" value=""/>
                                    <attribute name="Speed" value="83MHz"/>
                                    <attribute name="package" value="TBGA100"/>
                                    <attribute name="Memory_Format" value="FLASH"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
            </devicesets>
        </library>
    </drawing>
</eagle>
