<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle>
    <drawing>
        <library name="Upverter Library">
            <description>Upverter Parts Library

Created by Upverter.com</description>
            <packages>
                <package name="INVENSENSE_ICS-43434_0">
                    <description></description>
                </package>
            </packages>
            <symbols>
                <symbol name="INVENSENSE_ICS-43434_0_0">
                    <description></description>
                    <pin name="VDD"/>
                    <pin name="LR"/>
                    <pin name="SCK"/>
                    <pin name="SD"/>
                    <pin name="WS"/>
                    <pin name="GND"/>
                </symbol>
            </symbols>
            <devicesets>
                <deviceset prefix="MK" name="INVENSENSE_ICS-43434">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="INVENSENSE_ICS-43434_0_0"/>
                    </gates>
                    <devices>
                        <device name="INVENSENSE_ICS-43434_0_0" package="INVENSENSE_ICS-43434_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="WS"/>
                                <connect gate="G$0" pad="2" pin="LR"/>
                                <connect gate="G$0" pad="3" pin="GND"/>
                                <connect gate="G$0" pad="4" pin="SCK"/>
                                <connect gate="G$0" pad="5" pin="VDD"/>
                                <connect gate="G$0" pad="6" pin="SD"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="MPN" value="ICS-43434"/>
                                    <attribute name="package" value="MIC_SMT_2MM65_3MM5"/>
                                    <attribute name="digikey_description" value="MIC MEMS MULTI-MODE OMNI -26DB"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="digikey_part_number" value="1428-1066-1-ND"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="prefix" value="MK"/>
                                    <attribute name="MF" value="InvenSense"/>
                                    <attribute name="voltage" value=""/>
                                    <attribute name="temperature_range_low" value="− 40°C"/>
                                    <attribute name="datasheet" value="https://www.invensense.com/wp-content/uploads/2016/02/DS-000069-ICS-43434-v1.1.pdf"/>
                                    <attribute name="temperature_range_high" value="+85°C"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
            </devicesets>
        </library>
    </drawing>
</eagle>
